From 06ca36bbedeb5f75867bea2a2fdfe9a88b44e35f Mon Sep 17 00:00:00 2001
From: Tomi Valkeinen <tomi.valkeinen@ideasonboard.com>
Date: Fri, 29 Sep 2023 13:29:15 +0300
Subject: [PATCH 0650/1085] media: rp1: fe: Fix default mbus code

When pisp_fe_pad_set_fmt() is given an mbus code that CFE does not
support, it currently defaults to MEDIA_BUS_FMT_SBGGR10_1X10. This is
not correct, as FE does not support SBGGR10.

Set the default to MEDIA_BUS_FMT_SRGGB16_1X16 instead.

Signed-off-by: Tomi Valkeinen <tomi.valkeinen@ideasonboard.com>
---
 drivers/media/platform/raspberrypi/rp1_cfe/pisp_fe.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/platform/raspberrypi/rp1_cfe/pisp_fe.c
+++ b/drivers/media/platform/raspberrypi/rp1_cfe/pisp_fe.c
@@ -437,7 +437,7 @@ static int pisp_fe_pad_set_fmt(struct v4
 	case FE_OUTPUT1_PAD:
 		cfe_fmt = find_format_by_code(format->format.code);
 		if (!cfe_fmt || !(cfe_fmt->flags & CFE_FORMAT_FLAG_FE_OUT))
-			cfe_fmt = find_format_by_code(MEDIA_BUS_FMT_SBGGR10_1X10);
+			cfe_fmt = find_format_by_code(MEDIA_BUS_FMT_SRGGB16_1X16);
 
 		format->format.code = cfe_fmt->code;
 
