From: John Crispin <john@phrozen.org>
Subject: [PATCH] ath79: make ahb wifi work

Submitted-by: John Crispin <john@phrozen.org>
---
 arch/mips/ath79/common.c                      | 3 +++
 mips/include/asm/mach-ath79/ath79.h           | 1+
 1 file changed, 4 insertions(+)

--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -31,11 +31,13 @@ EXPORT_SYMBOL_GPL(ath79_ddr_freq);
 
 enum ath79_soc_type ath79_soc;
 unsigned int ath79_soc_rev;
+EXPORT_SYMBOL_GPL(ath79_soc_rev);
 
 void __iomem *ath79_pll_base;
 void __iomem *ath79_reset_base;
 EXPORT_SYMBOL_GPL(ath79_reset_base);
-static void __iomem *ath79_ddr_base;
+void __iomem *ath79_ddr_base;
+EXPORT_SYMBOL_GPL(ath79_ddr_base);
 static void __iomem *ath79_ddr_wb_flush_base;
 static void __iomem *ath79_ddr_pci_win_base;
 
--- a/arch/mips/include/asm/mach-ath79/ath79.h
+++ b/arch/mips/include/asm/mach-ath79/ath79.h
@@ -149,6 +149,7 @@ void ath79_ddr_wb_flush(unsigned int reg
 void ath79_ddr_set_pci_windows(void);
 
 extern void __iomem *ath79_pll_base;
+extern void __iomem *ath79_ddr_base;
 extern void __iomem *ath79_reset_base;
 
 static inline void ath79_pll_wr(unsigned reg, u32 val)
