From 28a72480cf1ae18abad4995aac293e1a1693776b Mon Sep 17 00:00:00 2001
From: Naushir Patuck <naush@raspberrypi.com>
Date: Thu, 14 Jan 2021 09:20:52 +0000
Subject: [PATCH 0275/1085] staging: vc04_services: ISP: Add colour denoise
 control

Add colour denoise control to the bcm2835 driver through a new v4l2
control: V4L2_CID_USER_BCM2835_ISP_CDN.

Add the accompanying MMAL configuration structure definitions as well.

Signed-off-by: Naushir Patuck <naush@raspberrypi.com>
---
 .../vc04_services/bcm2835-isp/bcm2835-isp-ctrls.h   |  5 +++++
 .../vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c    |  5 +++++
 .../vc04_services/vchiq-mmal/mmal-parameters.h      | 13 +++++++++++++
 3 files changed, 23 insertions(+)

--- a/drivers/staging/vc04_services/bcm2835-isp/bcm2835-isp-ctrls.h
+++ b/drivers/staging/vc04_services/bcm2835-isp/bcm2835-isp-ctrls.h
@@ -57,6 +57,11 @@ static const struct bcm2835_isp_custom_c
 		.size	= sizeof(struct bcm2835_isp_denoise),
 		.flags  = 0
 	}, {
+		.name	= "Colour Denoise",
+		.id	= V4L2_CID_USER_BCM2835_ISP_CDN,
+		.size	= sizeof(struct bcm2835_isp_cdn),
+		.flags  = 0
+	}, {
 		.name	= "Defective Pixel Correction",
 		.id	= V4L2_CID_USER_BCM2835_ISP_DPC,
 		.size	= sizeof(struct bcm2835_isp_dpc),
--- a/drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c
+++ b/drivers/staging/vc04_services/bcm2835-isp/bcm2835-v4l2-isp.c
@@ -766,6 +766,11 @@ static int bcm2835_isp_s_ctrl(struct v4l
 				    ctrl->p_new.p_u8,
 				    sizeof(struct bcm2835_isp_denoise));
 		break;
+	case V4L2_CID_USER_BCM2835_ISP_CDN:
+		ret = set_isp_param(node, MMAL_PARAMETER_CDN,
+				    ctrl->p_new.p_u8,
+				    sizeof(struct bcm2835_isp_cdn));
+		break;
 	case V4L2_CID_USER_BCM2835_ISP_SHARPEN:
 		ret = set_isp_param(node, MMAL_PARAMETER_SHARPEN,
 				    ctrl->p_new.p_u8,
--- a/drivers/staging/vc04_services/vchiq-mmal/mmal-parameters.h
+++ b/drivers/staging/vc04_services/vchiq-mmal/mmal-parameters.h
@@ -279,6 +279,8 @@ enum mmal_parameter_camera_type {
 	MMAL_PARAMETER_DPC,
 		/**< Tales a @ref MMAP_PARAMETER_GAMMA_T */
 	MMAL_PARAMETER_GAMMA,
+		/**< Takes a @ref MMAL_PARAMETER_CDN_T */
+	MMAL_PARAMETER_CDN,
 		/**< Takes a @ref MMAL_PARAMETER_BOOLEAN_T */
 	MMAL_PARAMETER_JPEG_IJG_SCALING,
 };
@@ -915,6 +917,17 @@ struct mmal_parameter_gamma {
 	u16 y[MMAL_NUM_GAMMA_PTS];
 };
 
+enum mmal_parameter_cdn_mode {
+	MMAL_PARAM_CDN_FAST = 0,
+	MMAL_PARAM_CDN_HIGH_QUALITY = 1,
+	MMAL_PARAM_CDN_DUMMY  = 0x7FFFFFFF
+};
+
+struct mmal_parameter_colour_denoise {
+	u32 enabled;
+	enum mmal_parameter_cdn_mode mode;
+};
+
 struct mmal_parameter_denoise {
 	u32 enabled;
 	u32 constant;
