From bef5018abb7cf94efafdc05087b4c998891ae4ec Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Mon, 17 Jan 2022 23:39:34 +0100
Subject: [PATCH v3 10/18] ARM: dts: qcom: add saw for l2 cache and kraitcc for
 ipq8064

Add saw compatible for l2 cache and kraitcc node for ipq8064 dtsi.
Also declare clock-output-names for acc0 and acc1 and qsb fixed clock
for the secondary mux.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Tested-by: Jonathan McDowell <noodles@earth.li>
---
 arch/arm/boot/dts/qcom/qcom-ipq8064.dtsi | 34 +++++++++++++++++++++++++++--
 1 file changed, 32 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/qcom/qcom-ipq8064.dtsi
+++ b/arch/arm/boot/dts/qcom/qcom-ipq8064.dtsi
@@ -302,6 +302,12 @@
 	};
 
 	clocks {
+		qsb: qsb {
+			compatible = "fixed-clock";
+			clock-frequency = <225000000>;
+			#clock-cells = <0>;
+		};
+
 		cxo_board: cxo_board {
 			compatible = "fixed-clock";
 			#clock-cells = <0>;
@@ -587,7 +593,7 @@
 		};
 
 		saw0: regulator@2089000 {
-			compatible = "qcom,saw2";
+			compatible = "qcom,saw2", "qcom,apq8064-saw2-v1.1-cpu", "syscon";
 			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;
 			regulator;
 		};
@@ -602,11 +608,27 @@
 		};
 
 		saw1: regulator@2099000 {
-			compatible = "qcom,saw2";
+			compatible = "qcom,saw2", "qcom,apq8064-saw2-v1.1-cpu", "syscon";
 			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;
 			regulator;
 		};
 
+		saw_l2: regulator@02012000 {
+			compatible = "qcom,saw2", "syscon";
+			reg = <0x02012000 0x1000>;
+			regulator;
+		};
+
+		kraitcc: clock-controller {
+			compatible = "qcom,krait-cc-v1";
+			clocks = <&gcc PLL9>, <&gcc PLL10>, <&gcc PLL12>,
+				 <&acc0>, <&acc1>, <&l2cc>, <&qsb>, <&pxo_board>;
+			clock-names = "hfpll0", "hfpll1", "hfpll_l2",
+				      "acpu0_aux", "acpu1_aux", "acpu_l2_aux",
+				      "qsb", "pxo";
+			#clock-cells = <1>;
+		};
+
 		nss_common: syscon@3000000 {
 			compatible = "syscon";
 			reg = <0x03000000 0x0000FFFF>;
