// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	model = "jjPlus JA76PF2";
	compatible = "jjplus,ja76pf2", "qca,ar7161";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_d2;
		led-failsafe = &led_d2;
		led-running = &led_d2;
		led-upgrade = &led_d2;
	};

	i2c {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		scl-gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;

		sensor@48 {
			compatible = "microchip,tcn75";
			reg = <0x48>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_d2: d2 {
			label = "green:d2";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		d3 {
			label = "green:d3";
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
		};

		d4 {
			label = "green:d4";
			gpios = <&gpio 3 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		sw1 {
			label = "sw1";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		sw2 {
			label = "sw2";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "rgmii";
	};

	phy4: ethernet-phy@4 {
		reg = <4>;
		phy-mode = "rgmii";
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_lan>;
	nvmem-cell-names = "mac-address";
	phy-handle = <&phy0>;
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_wan>;
	nvmem-cell-names = "mac-address";
	phy-handle = <&phy4>;
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "RedBoot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "loader";
				reg = <0x040000 0x020000>;
			};

			partition@60000 {
				label = "firmware";
				reg = <0x060000 0xf80000>;
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <IH_MAGIC_OKLI>;
			};

			partition@fe0000 {
				label = "FIS directory";
				reg = <0xfe0000 0x00f000>;
				read-only;
			};

			partition@fef000 {
				label = "RedBoot config";
				reg = <0xfef000 0x001000>;
				read-only;
			};

			partition@ff0000 {
				label = "Atheros Board Data";
				reg = <0xff0000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_wan: macaddr@1000 {
						reg = <0x1000 0x6>;
					};

					macaddr_lan: macaddr@1006 {
						reg = <0x1006 0x6>;
					};
				};
			};
		};
	};
};
