From 1172460e716784ac7e1049a537bdca8edbf97360 Mon Sep 17 00:00:00 2001
From: Miquel Raynal <miquel.raynal@bootlin.com>
Date: Fri, 15 Dec 2023 11:15:31 +0000
Subject: [PATCH] nvmem: Move and rename ->fixup_cell_info()

This hook is meant to be used by any provider and instantiating a layout
just for this is useless. Let's instead move this hook to the nvmem
device and add it to the config structure to be easily shared by the
providers.

While at moving this hook, rename it ->fixup_dt_cell_info() to clarify
its main intended purpose.

Signed-off-by: Miquel Raynal <miquel.raynal@bootlin.com>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20231215111536.316972-6-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/nvmem/core.c           |  6 +++---
 drivers/nvmem/imx-ocotp.c      | 11 +++--------
 drivers/nvmem/internals.h      |  2 ++
 drivers/nvmem/mtk-efuse.c      | 11 +++--------
 include/linux/nvmem-provider.h |  9 ++++-----
 5 files changed, 15 insertions(+), 24 deletions(-)

--- a/drivers/nvmem/core.c
+++ b/drivers/nvmem/core.c
@@ -674,7 +674,6 @@ static int nvmem_validate_keepouts(struc
 
 static int nvmem_add_cells_from_dt(struct nvmem_device *nvmem, struct device_node *np)
 {
-	struct nvmem_layout *layout = nvmem->layout;
 	struct device *dev = &nvmem->dev;
 	struct device_node *child;
 	const __be32 *addr;
@@ -704,8 +703,8 @@ static int nvmem_add_cells_from_dt(struc
 
 		info.np = of_node_get(child);
 
-		if (layout && layout->fixup_cell_info)
-			layout->fixup_cell_info(nvmem, layout, &info);
+		if (nvmem->fixup_dt_cell_info)
+			nvmem->fixup_dt_cell_info(nvmem, &info);
 
 		ret = nvmem_add_one_cell(nvmem, &info);
 		kfree(info.name);
@@ -894,6 +893,7 @@ struct nvmem_device *nvmem_register(cons
 
 	kref_init(&nvmem->refcnt);
 	INIT_LIST_HEAD(&nvmem->cells);
+	nvmem->fixup_dt_cell_info = config->fixup_dt_cell_info;
 
 	nvmem->owner = config->owner;
 	if (!nvmem->owner && config->dev->driver)
--- a/drivers/nvmem/imx-ocotp.c
+++ b/drivers/nvmem/imx-ocotp.c
@@ -583,17 +583,12 @@ static const struct of_device_id imx_oco
 };
 MODULE_DEVICE_TABLE(of, imx_ocotp_dt_ids);
 
-static void imx_ocotp_fixup_cell_info(struct nvmem_device *nvmem,
-				      struct nvmem_layout *layout,
-				      struct nvmem_cell_info *cell)
+static void imx_ocotp_fixup_dt_cell_info(struct nvmem_device *nvmem,
+					 struct nvmem_cell_info *cell)
 {
 	cell->read_post_process = imx_ocotp_cell_pp;
 }
 
-static struct nvmem_layout imx_ocotp_layout = {
-	.fixup_cell_info = imx_ocotp_fixup_cell_info,
-};
-
 static int imx_ocotp_probe(struct platform_device *pdev)
 {
 	struct device *dev = &pdev->dev;
@@ -619,7 +614,7 @@ static int imx_ocotp_probe(struct platfo
 	imx_ocotp_nvmem_config.size = 4 * priv->params->nregs;
 	imx_ocotp_nvmem_config.dev = dev;
 	imx_ocotp_nvmem_config.priv = priv;
-	imx_ocotp_nvmem_config.layout = &imx_ocotp_layout;
+	imx_ocotp_nvmem_config.fixup_dt_cell_info = &imx_ocotp_fixup_dt_cell_info;
 
 	priv->config = &imx_ocotp_nvmem_config;
 
--- a/drivers/nvmem/internals.h
+++ b/drivers/nvmem/internals.h
@@ -23,6 +23,8 @@ struct nvmem_device {
 	struct bin_attribute	eeprom;
 	struct device		*base_dev;
 	struct list_head	cells;
+	void (*fixup_dt_cell_info)(struct nvmem_device *nvmem,
+				   struct nvmem_cell_info *cell);
 	const struct nvmem_keepout *keepout;
 	unsigned int		nkeepout;
 	nvmem_reg_read_t	reg_read;
--- a/drivers/nvmem/mtk-efuse.c
+++ b/drivers/nvmem/mtk-efuse.c
@@ -45,9 +45,8 @@ static int mtk_efuse_gpu_speedbin_pp(voi
 	return 0;
 }
 
-static void mtk_efuse_fixup_cell_info(struct nvmem_device *nvmem,
-				      struct nvmem_layout *layout,
-				      struct nvmem_cell_info *cell)
+static void mtk_efuse_fixup_dt_cell_info(struct nvmem_device *nvmem,
+					 struct nvmem_cell_info *cell)
 {
 	size_t sz = strlen(cell->name);
 
@@ -61,10 +60,6 @@ static void mtk_efuse_fixup_cell_info(st
 		cell->read_post_process = mtk_efuse_gpu_speedbin_pp;
 }
 
-static struct nvmem_layout mtk_efuse_layout = {
-	.fixup_cell_info = mtk_efuse_fixup_cell_info,
-};
-
 static int mtk_efuse_probe(struct platform_device *pdev)
 {
 	struct device *dev = &pdev->dev;
@@ -91,7 +86,7 @@ static int mtk_efuse_probe(struct platfo
 	econfig.priv = priv;
 	econfig.dev = dev;
 	if (pdata->uses_post_processing)
-		econfig.layout = &mtk_efuse_layout;
+		econfig.fixup_dt_cell_info = &mtk_efuse_fixup_dt_cell_info;
 	nvmem = devm_nvmem_register(dev, &econfig);
 
 	return PTR_ERR_OR_ZERO(nvmem);
--- a/include/linux/nvmem-provider.h
+++ b/include/linux/nvmem-provider.h
@@ -83,6 +83,8 @@ struct nvmem_cell_info {
  * @cells:	Optional array of pre-defined NVMEM cells.
  * @ncells:	Number of elements in cells.
  * @add_legacy_fixed_of_cells:	Read fixed NVMEM cells from old OF syntax.
+ * @fixup_dt_cell_info: Will be called before a cell is added. Can be
+ *		used to modify the nvmem_cell_info.
  * @keepout:	Optional array of keepout ranges (sorted ascending by start).
  * @nkeepout:	Number of elements in the keepout array.
  * @type:	Type of the nvmem storage
@@ -113,6 +115,8 @@ struct nvmem_config {
 	const struct nvmem_cell_info	*cells;
 	int			ncells;
 	bool			add_legacy_fixed_of_cells;
+	void (*fixup_dt_cell_info)(struct nvmem_device *nvmem,
+				   struct nvmem_cell_info *cell);
 	const struct nvmem_keepout *keepout;
 	unsigned int		nkeepout;
 	enum nvmem_type		type;
@@ -158,8 +162,6 @@ struct nvmem_cell_table {
  * @of_match_table:	Open firmware match table.
  * @add_cells:		Called to populate the layout using
  *			nvmem_add_one_cell().
- * @fixup_cell_info:	Will be called before a cell is added. Can be
- *			used to modify the nvmem_cell_info.
  * @owner:		Pointer to struct module.
  * @node:		List node.
  *
@@ -172,9 +174,6 @@ struct nvmem_layout {
 	const char *name;
 	const struct of_device_id *of_match_table;
 	int (*add_cells)(struct device *dev, struct nvmem_device *nvmem);
-	void (*fixup_cell_info)(struct nvmem_device *nvmem,
-				struct nvmem_layout *layout,
-				struct nvmem_cell_info *cell);
 
 	/* private */
 	struct module *owner;
