--- a/src/mpoad/mpcd.8
+++ b/src/mpoad/mpcd.8
@@ -28,7 +28,7 @@ mpcd \- ATM MPOA (Multi\-Protocol Over A
 .B ]]
 .SH DESCRIPTION
 MPOA client
-.SM(MPC) is responsible for creating and receiving
+.SM (MPC) is responsible for creating and receiving
 internetwork layer shortcuts. Using these shortcuts MPCs forward
 unicast internetwork layer packets effectively over ATM without need
 for routing protocols.
@@ -43,7 +43,7 @@ accepts shortcuts and packets arriving o
 shortcuts is done with the help of
 .SM MPOA
 server
-.SM(MPS).
+.SM (MPS).
 .PP
 Just as the Linux
 .SM LAN
--- a/src/led/zeppelin.8
+++ b/src/led/zeppelin.8
@@ -99,7 +99,7 @@ Ring and ATM parts of the ELAN, so using
 recommended. Token Ring support has received less testing than its
 Ethernet counterpart.
 .SH FILES
-.IP \fI/var/run/lec[interface number].pid\fP
+.IP \fI/var/run/lec[interface\ number].pid\fP
 The file containing the process id of zeppelin.
 .SH BUGS
 John Bonham died 1980 and Led Zeppelin broke.
--- a/src/sigd/atmsigd.conf.4
+++ b/src/sigd/atmsigd.conf.4
@@ -125,7 +125,7 @@ a comment. The `#' character cannot be e
 .P
 If an option is specified in \fBatmsigd.conf\fP and on the command
 line, the command line has priority.
-.COMPATIBILITY
+.SH COMPATIBILITY
 Certain options used by past versions of \fBatmsigd\fP but no longer documented
 on the man page are still recognized and supported, but they also yield a
 warning message. Future versions of \fBatmsigd\fP will not recognize those
--- a/src/arpd/io.c
+++ b/src/arpd/io.c
@@ -277,7 +277,8 @@ static void accept_new(void)
     struct atm_qos qos;
     ENTRY *entry;
     VCC *vcc;
-    int fd,len,size,error;
+    int fd,error;
+    socklen_t len,size;
 
     len = sizeof(addr);
     if ((fd = accept(incoming,(struct sockaddr *) &addr,&len)) < 0) {
@@ -614,7 +615,8 @@ int ip_itf_info(int number,uint32_t *ip,
 
 int get_local(int fd,struct sockaddr_atmsvc *addr)
 {
-    int length,result;
+    int result;
+    size_t length;
 
     length = sizeof(struct sockaddr_atmsvc);
     result = getsockname(fd,(struct sockaddr *) addr,&length);
--- a/src/arpd/table.c
+++ b/src/arpd/table.c
@@ -101,7 +101,8 @@ static void dump_vcc(VCC *vcc)
     char addr_buf[MAX_ATM_ADDR_LEN+1];
     char qos_buf[MAX_ATM_QOS_LEN+1];
     struct atm_qos qos;
-    int size,sndbuf;
+    int sndbuf;
+    socklen_t size;
 
     size = sizeof(addr);
     if (getpeername(vcc->fd,(struct sockaddr *) &addr,&size) < 0) {
--- a/src/ilmid/asn1/asn_int.c
+++ b/src/ilmid/asn1/asn_int.c
@@ -185,7 +185,7 @@ FILE* f _AND_
 AsnInt* v _AND_
 unsigned short int indent)
 {
-    fprintf(f,"%d", *v);
+    fprintf(f,"%ld", *v);
 } 
 
 
@@ -370,5 +370,5 @@ FILE* f _AND_
 UAsnInt* v _AND_
 unsigned short int indent)
 {
-    fprintf(f,"%u", *v);
+    fprintf(f,"%lu", *v);
 } 
--- a/src/ilmid/asn1/asn_oid.c
+++ b/src/ilmid/asn1/asn_oid.c
@@ -127,7 +127,7 @@ unsigned short int indent)
     if (firstArcNum > 2)
         firstArcNum = 2;
 
-    fprintf(f,"%u %u", firstArcNum, arcNum - (firstArcNum * 40));
+    fprintf(f,"%d %lu", firstArcNum, arcNum - (firstArcNum * 40));
 
     for (; i < v->octetLen ; )
     {
@@ -136,7 +136,7 @@ unsigned short int indent)
 
         arcNum = (arcNum << 7) + (v->octs[i] & 0x7f);
         i++;
-        fprintf(f," %u", arcNum);
+        fprintf(f," %lu", arcNum);
     }
     fprintf(f,"}");
 
--- a/src/lane/connect.c
+++ b/src/lane/connect.c
@@ -258,7 +258,8 @@ static int
 data_handler(const Event_t *event, void *funcdata)
 {
   Conn_t *tmp, *newconn;
-  int fd, nbytes;
+  int fd;
+  socklen_t nbytes;
   static char buffer[BUFSIZE];
   LaneControl_t *ctmp;
   struct sockaddr_atmsvc addr;
--- a/src/lane/connect_bus.c
+++ b/src/lane/connect_bus.c
@@ -170,7 +170,8 @@ static int
 data_handler(const Event_t *event, void *funcdata)
 {
   Conn_t *tmp, *newconn;
-  int fd, nbytes;
+  int fd;
+  socklen_t nbytes;
   static char buffer[BUFSIZE];
   struct sockaddr_atmsvc addr;
 
--- a/src/lane/lane_atm.c
+++ b/src/lane/lane_atm.c
@@ -138,7 +138,7 @@ atm_connect_back(const AtmAddr_t *our_ad
   struct atm_blli blli;
   struct atm_qos qos;
   int fd, ret;
-  int len = sizeof(address);
+  socklen_t len = sizeof(address);
   
   fd = socket(PF_ATMSVC, SOCK_DGRAM, 0);
   if (fd <0) {
--- a/src/lane/lecs.c
+++ b/src/lane/lecs.c
@@ -119,7 +119,7 @@ int main(int argc, char **argv)
   int just_dump=0;
   fd_set fds;
   struct sockaddr_atmsvc client;
-  int len;
+  socklen_t len;
   unsigned char buffer[P_SIZE];
 
   while(i!=-1) {
--- a/src/lib/ans.c
+++ b/src/lib/ans.c
@@ -41,7 +41,7 @@
 static int ans(const char *text,int wanted,void *result,int res_len)
 {
     unsigned char answer[MAX_ANSWER];
-    unsigned char name[MAX_NAME];
+    char name[MAX_NAME];
     unsigned char *pos,*data,*found;
     int answer_len,name_len,data_len,found_len;
     int questions,answers;
--- a/src/lib/sdu2cell.c
+++ b/src/lib/sdu2cell.c
@@ -15,7 +15,8 @@ int sdu2cell(int s,int sizes,const int *
 {
     struct atm_qos qos;
     int trailer,total,cells;
-    int size,i;
+    int i;
+    socklen_t size;
 
     size = sizeof(qos);
     if (getsockopt(s,SOL_AAL,SO_ATMQOS,&qos,&size) < 0) return -1;
--- a/src/lib/unix.c
+++ b/src/lib/unix.c
@@ -63,8 +63,8 @@ int un_attach(const char *path)
 int un_recv_connect(int s,void *buf,int size)
 {
     struct sockaddr_un addr;
-    int addr_size;
     int len;
+    socklen_t addr_size;
 
     addr_size = sizeof(addr);
     len = recvfrom(s,buf,size,0,(struct sockaddr *) &addr,&addr_size);
--- a/src/maint/atmtcp.c
+++ b/src/maint/atmtcp.c
@@ -817,7 +817,8 @@ int main(int argc,char **argv)
 	}
 	else if (!strcmp(ARG,"listen") ||
 	  (do_background = !strcmp(ARG,"listen-bg"))) {
-	    int fd,port,addr_len;
+	    int fd,port;
+	    socklen_t addr_len;
 	    int *fd2 = alloc_t(int);
 
 	    if ((fd = socket(PF_INET,SOCK_STREAM,0)) < 0) {
--- a/src/maint/hediag.c
+++ b/src/maint/hediag.c
@@ -1,6 +1,7 @@
 #include <stdio.h>
 #include <stdlib.h>
 #include <unistd.h>
+#include <string.h>
 #include <sys/ioctl.h>
 #include <sys/types.h>
 #include <sys/socket.h>
--- a/src/mpoad/io.c
+++ b/src/mpoad/io.c
@@ -521,7 +521,8 @@ static int msg_from_mps(int slot)
 static int accept_conn(int slot)
 {
         struct sockaddr_atmsvc sa;
-        int i, new_fd, sa_len;
+        int i, new_fd;
+        socklen_t sa_len;
 
         sa_len = sizeof(sa);
         new_fd = accept(fds[slot].fd, (struct sockaddr *)&sa, &sa_len);
--- a/src/sigd/io.c
+++ b/src/sigd/io.c
@@ -355,7 +355,7 @@ int get_pvc(int itf,int *vci)
     error = 0;
     if (bind(s,(struct sockaddr *) &addr,sizeof(addr)) < 0) error = errno;
     else {
-	int size;
+	socklen_t size;
 
 	size = sizeof(addr);
 	if (getsockname(s,(struct sockaddr *) &addr,&size) < 0)
--- a/src/test/ttcp.c
+++ b/src/test/ttcp.c
@@ -92,7 +92,8 @@ struct sockaddr_in frominet;
 struct sockaddr_atmsvc satm;
 struct atm_qos qos;
 
-int domain, fromlen;
+int domain;
+socklen_t fromlen;
 int fd;				/* fd of network socket */
 
 int buflen = 8 * 1024;		/* length of buffer */
@@ -466,7 +467,7 @@ int no_check = 0;
 	    
 	    {
 		struct sockaddr_atmsvc peer;
-		int peerlen = sizeof(peer);
+		socklen_t peerlen = sizeof(peer);
 		if (getpeername(fd, (struct sockaddr *) &peer, 
 				&peerlen) < 0) {
 		    err("getpeername");
@@ -498,7 +499,7 @@ int no_check = 0;
     /* set socket buffer size */
 #if defined(SO_SNDBUF) || defined(SO_RCVBUF)
     if (sockbufsize) {
-	int len;
+	socklen_t len;
 
 	if (trans) {
 	    /* set send socket buffer if we are transmitting */    
@@ -663,7 +664,7 @@ int no_check = 0;
     exit(0);
 
   usage:
-    fprintf(stderr, Usage);
+    fprintf(stderr, "%s", Usage);
     exit(1);
 }
 
--- a/src/arpd/arp.c
+++ b/src/arpd/arp.c
@@ -17,6 +17,7 @@
 #include <netinet/in.h> /* for ntohs, etc. */
 #define _LINUX_NETDEVICE_H /* very crude hack for glibc2 */
 #include <linux/types.h>
+#include <linux/if.h>
 #include <linux/if_arp.h>
 #include <linux/if_ether.h>
 #include <atm.h>
--- a/src/arpd/itf.c
+++ b/src/arpd/itf.c
@@ -14,6 +14,7 @@
 #include <sys/socket.h>
 #define _LINUX_NETDEVICE_H /* glibc2 */
 #include <linux/types.h>
+#include <linux/if.h>
 #include <linux/if_arp.h>
 
 #include "atmd.h"
--- a/src/maint/atmdump.c
+++ b/src/maint/atmdump.c
@@ -14,6 +14,7 @@
 #include <sys/types.h>
 #include <sys/time.h>
 #include <sys/socket.h>
+#include <linux/sockios.h>
 #include <netinet/in.h> /* for htonl and ntohl */
 #include <atm.h>
 
--- a/src/maint/saaldump.c
+++ b/src/maint/saaldump.c
@@ -15,6 +15,7 @@
 #include <sys/time.h>
 #include <sys/types.h>
 #include <sys/socket.h>
+#include <linux/sockios.h>
 #include <atm.h>
 
 #include "pdu.h"
