From bc6a6a4ec6c28467683121cc165e5681b4acdf8d Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Tue, 27 Aug 2024 23:04:53 +0200
Subject: [PATCH 3/3] thermal: Add support for Airoha EN7581 thermal sensor

Add support for Airoha EN7581 thermal sensor. This provide support for
reading the CPU or SoC Package sensor and to setup trip points for hot
and critical condition. An interrupt is fired to react on this and
doesn't require passive poll to read the temperature.

The thermal regs provide a way to read the ADC value from an external
register placed in the Chip SCU regs. Monitor will read this value and
fire an interrupt if the trip condition configured is reached.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/thermal/Kconfig          |   9 +
 drivers/thermal/Makefile         |   1 +
 drivers/thermal/airoha_thermal.c | 482 +++++++++++++++++++++++++++++++
 3 files changed, 492 insertions(+)
 create mode 100644 drivers/thermal/airoha_thermal.c

--- a/drivers/thermal/Kconfig
+++ b/drivers/thermal/Kconfig
@@ -317,6 +317,15 @@ config QORIQ_THERMAL
 	  cpufreq is used as the cooling device to throttle CPUs when the
 	  passive trip is crossed.
 
+config AIROHA_THERMAL
+	tristate "Airoha thermal sensor driver"
+	depends on ARCH_AIROHA || COMPILE_TEST
+	depends on MFD_SYSCON
+	depends on OF
+	help
+	  Enable this to plug the Airoha thermal sensor driver into the Linux
+	  thermal framework.
+
 config SPEAR_THERMAL
 	tristate "SPEAr thermal sensor driver"
 	depends on PLAT_SPEAR || COMPILE_TEST
--- a/drivers/thermal/Makefile
+++ b/drivers/thermal/Makefile
@@ -34,6 +34,7 @@ obj-$(CONFIG_K3_THERMAL)	+= k3_bandgap.o
 # platform thermal drivers
 obj-y				+= broadcom/
 obj-$(CONFIG_THERMAL_MMIO)		+= thermal_mmio.o
+obj-$(CONFIG_AIROHA_THERMAL)	+= airoha_thermal.o
 obj-$(CONFIG_SPEAR_THERMAL)	+= spear_thermal.o
 obj-$(CONFIG_SUN8I_THERMAL)     += sun8i_thermal.o
 obj-$(CONFIG_ROCKCHIP_THERMAL)	+= rockchip_thermal.o
--- /dev/null
+++ b/drivers/thermal/airoha_thermal.c
@@ -0,0 +1,482 @@
+// SPDX-License-Identifier: GPL-2.0-or-later
+
+#include <linux/module.h>
+#include <linux/bitfield.h>
+#include <linux/delay.h>
+#include <linux/interrupt.h>
+#include <linux/mfd/syscon.h>
+#include <linux/of.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+#include <linux/thermal.h>
+
+/* SCU regs */
+#define EN7581_PLLRG_PROTECT			0x268
+#define EN7581_PWD_TADC				0x2ec
+#define   EN7581_MUX_TADC			GENMASK(3, 1)
+#define EN7581_DOUT_TADC			0x2f8
+#define   EN7581_DOUT_TADC_MASK			GENMASK(15, 0)
+
+/* PTP_THERMAL regs */
+#define EN7581_TEMPMONCTL0			0x800
+#define   EN7581_SENSE3_EN			BIT(3)
+#define   EN7581_SENSE2_EN			BIT(2)
+#define   EN7581_SENSE1_EN			BIT(1)
+#define   EN7581_SENSE0_EN			BIT(0)
+#define EN7581_TEMPMONCTL1			0x804
+/* period unit calculated in BUS clock * 256 scaling-up */
+#define   EN7581_PERIOD_UNIT			GENMASK(9, 0)
+#define EN7581_TEMPMONCTL2			0x808
+#define   EN7581_FILT_INTERVAL			GENMASK(25, 16)
+#define   EN7581_SEN_INTERVAL			GENMASK(9, 0)
+#define EN7581_TEMPMONINT			0x80C
+#define   EN7581_STAGE3_INT_EN			BIT(31)
+#define   EN7581_STAGE2_INT_EN			BIT(30)
+#define   EN7581_STAGE1_INT_EN			BIT(29)
+#define   EN7581_FILTER_INT_EN_3		BIT(28)
+#define   EN7581_IMMD_INT_EN3			BIT(27)
+#define   EN7581_NOHOTINTEN3			BIT(26)
+#define   EN7581_HOFSINTEN3			BIT(25)
+#define   EN7581_LOFSINTEN3			BIT(24)
+#define   EN7581_HINTEN3			BIT(23)
+#define   EN7581_CINTEN3			BIT(22)
+#define   EN7581_FILTER_INT_EN_2		BIT(21)
+#define   EN7581_FILTER_INT_EN_1		BIT(20)
+#define   EN7581_FILTER_INT_EN_0		BIT(19)
+#define   EN7581_IMMD_INT_EN2			BIT(18)
+#define   EN7581_IMMD_INT_EN1			BIT(17)
+#define   EN7581_IMMD_INT_EN0			BIT(16)
+#define   EN7581_TIME_OUT_INT_EN		BIT(15)
+#define   EN7581_NOHOTINTEN2			BIT(14)
+#define   EN7581_HOFSINTEN2			BIT(13)
+#define   EN7581_LOFSINTEN2			BIT(12)
+#define   EN7581_HINTEN2			BIT(11)
+#define   EN7581_CINTEN2			BIT(10)
+#define   EN7581_NOHOTINTEN1			BIT(9)
+#define   EN7581_HOFSINTEN1			BIT(8)
+#define   EN7581_LOFSINTEN1			BIT(7)
+#define   EN7581_HINTEN1			BIT(6)
+#define   EN7581_CINTEN1			BIT(5)
+#define   EN7581_NOHOTINTEN0			BIT(4)
+/* Similar to COLD and HOT also these seems to be swapped in documentation */
+#define   EN7581_LOFSINTEN0			BIT(3) /* In documentation: BIT(2) */
+#define   EN7581_HOFSINTEN0			BIT(2) /* In documentation: BIT(3) */
+/* It seems documentation have these swapped as the HW
+ * - Fire BIT(1) when lower than EN7581_COLD_THRE
+ * - Fire BIT(0) and BIT(5) when higher than EN7581_HOT2NORMAL_THRE or
+ *     EN7581_HOT_THRE
+ */
+#define   EN7581_CINTEN0			BIT(1) /* In documentation: BIT(0) */
+#define   EN7581_HINTEN0			BIT(0) /* In documentation: BIT(1) */
+#define EN7581_TEMPMONINTSTS			0x810
+#define   EN7581_STAGE3_INT_STAT		BIT(31)
+#define   EN7581_STAGE2_INT_STAT		BIT(30)
+#define   EN7581_STAGE1_INT_STAT		BIT(29)
+#define   EN7581_FILTER_INT_STAT_3		BIT(28)
+#define   EN7581_IMMD_INT_STS3			BIT(27)
+#define   EN7581_NOHOTINTSTS3			BIT(26)
+#define   EN7581_HOFSINTSTS3			BIT(25)
+#define   EN7581_LOFSINTSTS3			BIT(24)
+#define   EN7581_HINTSTS3			BIT(23)
+#define   EN7581_CINTSTS3			BIT(22)
+#define   EN7581_FILTER_INT_STAT_2		BIT(21)
+#define   EN7581_FILTER_INT_STAT_1		BIT(20)
+#define   EN7581_FILTER_INT_STAT_0		BIT(19)
+#define   EN7581_IMMD_INT_STS2			BIT(18)
+#define   EN7581_IMMD_INT_STS1			BIT(17)
+#define   EN7581_IMMD_INT_STS0			BIT(16)
+#define   EN7581_TIME_OUT_INT_STAT		BIT(15)
+#define   EN7581_NOHOTINTSTS2			BIT(14)
+#define   EN7581_HOFSINTSTS2			BIT(13)
+#define   EN7581_LOFSINTSTS2			BIT(12)
+#define   EN7581_HINTSTS2			BIT(11)
+#define   EN7581_CINTSTS2			BIT(10)
+#define   EN7581_NOHOTINTSTS1			BIT(9)
+#define   EN7581_HOFSINTSTS1			BIT(8)
+#define   EN7581_LOFSINTSTS1			BIT(7)
+#define   EN7581_HINTSTS1			BIT(6)
+#define   EN7581_CINTSTS1			BIT(5)
+#define   EN7581_NOHOTINTSTS0			BIT(4)
+/* Similar to COLD and HOT also these seems to be swapped in documentation */
+#define   EN7581_LOFSINTSTS0			BIT(3) /* In documentation: BIT(2) */
+#define   EN7581_HOFSINTSTS0			BIT(2) /* In documentation: BIT(3) */
+/* It seems documentation have these swapped as the HW
+ * - Fire BIT(1) when lower than EN7581_COLD_THRE
+ * - Fire BIT(0) and BIT(5) when higher than EN7581_HOT2NORMAL_THRE or
+ *     EN7581_HOT_THRE
+ *
+ * To clear things, we swap the define but we keep them documented here.
+ */
+#define   EN7581_CINTSTS0			BIT(1) /* In documentation: BIT(0) */
+#define   EN7581_HINTSTS0			BIT(0) /* In documentation: BIT(1)*/
+/* Monitor will take the bigger threshold between HOT2NORMAL and HOT
+ * and will fire both HOT2NORMAL and HOT interrupt when higher than the 2
+ *
+ * It has also been observed that not setting HOT2NORMAL makes the monitor
+ * treat COLD threshold as HOT2NORMAL.
+ */
+#define EN7581_TEMPH2NTHRE			0x824
+/* It seems HOT2NORMAL is actually NORMAL2HOT */
+#define   EN7581_HOT2NORMAL_THRE		GENMASK(11, 0)
+#define EN7581_TEMPHTHRE			0x828
+#define   EN7581_HOT_THRE			GENMASK(11, 0)
+/* Monitor will use this as HOT2NORMAL (fire interrupt when lower than...)*/
+#define EN7581_TEMPCTHRE			0x82c
+#define   EN7581_COLD_THRE			GENMASK(11, 0)
+/* Also LOW and HIGH offset register are swapped */
+#define EN7581_TEMPOFFSETL			0x830 /* In documentation: 0x834 */
+#define   EN7581_LOW_OFFSET			GENMASK(11, 0)
+#define EN7581_TEMPOFFSETH			0x834 /* In documentation: 0x830 */
+#define   EN7581_HIGH_OFFSET			GENMASK(11, 0)
+#define EN7581_TEMPMSRCTL0			0x838
+#define   EN7581_MSRCTL3			GENMASK(11, 9)
+#define   EN7581_MSRCTL2			GENMASK(8, 6)
+#define   EN7581_MSRCTL1			GENMASK(5, 3)
+#define   EN7581_MSRCTL0			GENMASK(2, 0)
+#define EN7581_TEMPADCVALIDADDR			0x878
+#define   EN7581_ADC_VALID_ADDR			GENMASK(31, 0)
+#define EN7581_TEMPADCVOLTADDR			0x87c
+#define   EN7581_ADC_VOLT_ADDR			GENMASK(31, 0)
+#define EN7581_TEMPRDCTRL			0x880
+/*
+ * NOTICE: AHB have this set to 0 by default. Means that
+ * the same addr is used for ADC volt and valid reading.
+ * In such case, VALID ADDR is used and volt addr is ignored.
+ */
+#define   EN7581_RD_CTRL_DIFF			BIT(0)
+#define EN7581_TEMPADCVALIDMASK			0x884
+#define   EN7581_ADV_RD_VALID_POLARITY		BIT(5)
+#define   EN7581_ADV_RD_VALID_POS		GENMASK(4, 0)
+#define EN7581_TEMPADCVOLTAGESHIFT		0x888
+#define   EN7581_ADC_VOLTAGE_SHIFT		GENMASK(4, 0)
+/*
+ * Same values for each CTL.
+ * Can operate in:
+ * - 1 sample
+ * - 2 sample and make average of them
+ * - 4,6,10,16 sample, drop max and min and make avgerage of them
+ */
+#define   EN7581_MSRCTL_1SAMPLE			0x0
+#define   EN7581_MSRCTL_AVG2SAMPLE		0x1
+#define   EN7581_MSRCTL_4SAMPLE_MAX_MIX_AVG2	0x2
+#define   EN7581_MSRCTL_6SAMPLE_MAX_MIX_AVG4	0x3
+#define   EN7581_MSRCTL_10SAMPLE_MAX_MIX_AVG8	0x4
+#define   EN7581_MSRCTL_18SAMPLE_MAX_MIX_AVG16	0x5
+#define EN7581_TEMPAHBPOLL			0x840
+#define   EN7581_ADC_POLL_INTVL			GENMASK(31, 0)
+/* PTPSPARE0,2 reg are used to store efuse info for calibrated temp offset */
+#define EN7581_EFUSE_TEMP_OFFSET_REG		0xf20 /* PTPSPARE0 */
+#define   EN7581_EFUSE_TEMP_OFFSET		GENMASK(31, 16)
+#define EN7581_PTPSPARE1			0xf24 /* PTPSPARE1 */
+#define EN7581_EFUSE_TEMP_CPU_SENSOR_REG	0xf28 /* PTPSPARE2 */
+
+#define EN7581_SLOPE_X100_DIO_DEFAULT		5645
+#define EN7581_SLOPE_X100_DIO_AVS		5645
+
+#define EN7581_INIT_TEMP_CPK_X10		300
+#define EN7581_INIT_TEMP_FTK_X10		620
+#define EN7581_INIT_TEMP_NONK_X10		550
+
+#define EN7581_SCU_THERMAL_PROTECT_KEY		0x12
+#define EN7581_SCU_THERMAL_MUX_DIODE1		0x7
+
+/* Convert temp to raw value as read from ADC	((((temp / 100) - init) * slope) / 1000) + offset */
+#define TEMP_TO_RAW(priv, tz, temp)		((((((temp) / 100) - (priv)->init_temp) * \
+						  thermal_zone_get_slope(tz)) / 1000) + \
+						  thermal_zone_get_offset(tz))
+
+/* Convert raw to temp				((((temp - offset) * 1000) / slope + init) * 100) */
+#define RAW_TO_TEMP(priv, tz, raw)		(((((raw) - thermal_zone_get_offset(tz)) * 1000) / \
+						  thermal_zone_get_slope(tz) + \
+						  (priv)->init_temp) * 100)
+
+struct airoha_thermal_priv {
+	void __iomem *base;
+	struct regmap *chip_scu;
+	struct resource scu_adc_res;
+
+	struct thermal_zone_device *tz;
+	int init_temp;
+};
+
+static int airoha_get_thermal_ADC(struct airoha_thermal_priv *priv)
+{
+	u32 val;
+
+	regmap_read(priv->chip_scu, EN7581_DOUT_TADC, &val);
+	return FIELD_GET(EN7581_DOUT_TADC_MASK, val);
+}
+
+static void airoha_init_thermal_ADC_mode(struct airoha_thermal_priv *priv)
+{
+	u32 adc_mux, pllrg;
+
+	/* Save PLLRG current value */
+	regmap_read(priv->chip_scu, EN7581_PLLRG_PROTECT, &pllrg);
+
+	/* Give access to thermal regs */
+	regmap_write(priv->chip_scu, EN7581_PLLRG_PROTECT, EN7581_SCU_THERMAL_PROTECT_KEY);
+	adc_mux = FIELD_PREP(EN7581_MUX_TADC, EN7581_SCU_THERMAL_MUX_DIODE1);
+	regmap_write(priv->chip_scu, EN7581_PWD_TADC, adc_mux);
+
+	/* Restore PLLRG value on exit */
+	regmap_write(priv->chip_scu, EN7581_PLLRG_PROTECT, pllrg);
+}
+
+static int airoha_thermal_get_temp(struct thermal_zone_device *tz, int *temp)
+{
+	struct airoha_thermal_priv *priv = thermal_zone_device_priv(tz);
+	int min, max, avg_temp, temp_adc;
+	int i;
+
+	/* Get the starting temp */
+	temp_adc = airoha_get_thermal_ADC(priv);
+	min = temp_adc;
+	max = temp_adc;
+	avg_temp = temp_adc;
+
+	/* Make 5 more measurement and average the temp ADC difference */
+	for (i = 0; i < 5; i++) {
+		temp_adc = airoha_get_thermal_ADC(priv);
+		avg_temp += temp_adc;
+		if (temp_adc > max)
+			max = temp_adc;
+		if (temp_adc < min)
+			min = temp_adc;
+	}
+	avg_temp = avg_temp - max - min;
+	avg_temp /= 4;
+
+	*temp = RAW_TO_TEMP(priv, tz, avg_temp);
+	return 0;
+}
+
+static int airoha_thermal_set_trips(struct thermal_zone_device *tz, int low,
+				    int high)
+{
+	struct airoha_thermal_priv *priv = thermal_zone_device_priv(tz);
+
+	if (high != INT_MAX) {
+		/* Validate high and clamp them a sane value */
+		if (high > RAW_TO_TEMP(priv, tz, FIELD_MAX(EN7581_DOUT_TADC_MASK)))
+			high = 110000;
+
+		/* We offset the high temp of 1°C to trigger correct event */
+		writel(TEMP_TO_RAW(priv, tz, high) >> 4,
+		       priv->base + EN7581_TEMPOFFSETH);
+	}
+
+	if (low != -INT_MAX) {
+		/* Validate low and clamp them to a sane value */
+		if (low < RAW_TO_TEMP(priv, tz, 0))
+			low = -33000;
+
+		/* We offset the low temp of 1°C to trigger correct event */
+		writel(TEMP_TO_RAW(priv, tz, low) >> 4,
+		       priv->base + EN7581_TEMPOFFSETL);
+	}
+
+	/* Enable sensor 0 monitor */
+	writel(EN7581_SENSE0_EN, priv->base + EN7581_TEMPMONCTL0);
+
+	return 0;
+}
+
+static const struct thermal_zone_device_ops thdev_ops = {
+	.get_temp = airoha_thermal_get_temp,
+	.set_trips = airoha_thermal_set_trips,
+};
+
+static irqreturn_t airoha_thermal_irq(int irq, void *data)
+{
+	struct airoha_thermal_priv *priv = data;
+	enum thermal_notify_event event;
+	u32 status;
+
+	status = readl(priv->base + EN7581_TEMPMONINTSTS);
+	switch (status & (EN7581_HOFSINTSTS0 | EN7581_LOFSINTSTS0)) {
+	case EN7581_HOFSINTSTS0:
+		event = THERMAL_TRIP_VIOLATED;
+		break;
+	case EN7581_LOFSINTSTS0:
+		event = THERMAL_EVENT_UNSPECIFIED;
+		break;
+	default:
+		goto exit;
+	}
+
+	thermal_zone_device_update(priv->tz, event);
+
+exit:
+	/* reset interrupt */
+	writel(status, priv->base + EN7581_TEMPMONINTSTS);
+
+	return IRQ_HANDLED;
+}
+
+static void airoha_thermal_setup_adc_val(struct device *dev,
+					 struct airoha_thermal_priv *priv,
+					 struct thermal_zone_params *tzp)
+{
+	u32 efuse_calib_info, cpu_sensor;
+
+	/* Setup thermal sensor to ADC mode and setup the mux to DIODE1 */
+	airoha_init_thermal_ADC_mode(priv);
+	/* sleep 10 ms for ADC to enable */
+	usleep_range(10 * USEC_PER_MSEC, 11 * USEC_PER_MSEC);
+
+	efuse_calib_info = readl(priv->base + EN7581_EFUSE_TEMP_OFFSET_REG);
+	if (efuse_calib_info) {
+		tzp->offset = FIELD_GET(EN7581_EFUSE_TEMP_OFFSET, efuse_calib_info);
+		/* Different slope are applied if the sensor is used for CPU or for package */
+		cpu_sensor = readl(priv->base + EN7581_EFUSE_TEMP_CPU_SENSOR_REG);
+		if (cpu_sensor) {
+			tzp->slope = EN7581_SLOPE_X100_DIO_DEFAULT;
+			priv->init_temp = EN7581_INIT_TEMP_FTK_X10;
+		} else {
+			tzp->slope = EN7581_SLOPE_X100_DIO_AVS;
+			priv->init_temp = EN7581_INIT_TEMP_CPK_X10;
+		}
+	} else {
+		tzp->offset = airoha_get_thermal_ADC(priv);
+		tzp->slope = EN7581_SLOPE_X100_DIO_DEFAULT;
+		priv->init_temp = EN7581_INIT_TEMP_NONK_X10;
+		dev_info(dev, "missing thermal calibrarion EFUSE, using non calibrated value\n");
+	}
+}
+
+static void airoha_thermal_setup_monitor(struct airoha_thermal_priv *priv)
+{
+	/* Set measure mode */
+	writel(FIELD_PREP(EN7581_MSRCTL0, EN7581_MSRCTL_6SAMPLE_MAX_MIX_AVG4),
+	       priv->base + EN7581_TEMPMSRCTL0);
+
+	/*
+	 * Configure ADC valid reading addr
+	 * The AHB temp monitor system doesn't have direct access to the
+	 * thermal sensor. It does instead work by providing all kind of
+	 * address to configure how to access and setup an ADC for the
+	 * sensor. EN7581 supports only one sensor hence the
+	 * implementation is greatly simplified but the AHB supports
+	 * up to 4 different sensor from the same ADC that can be
+	 * switched by tuning the ADC mux or wiriting address.
+	 *
+	 * We set valid instead of volt as we don't enable valid/volt
+	 * split reading and AHB read valid addr in such case.
+	 */
+	writel(priv->scu_adc_res.start + EN7581_DOUT_TADC,
+	       priv->base + EN7581_TEMPADCVALIDADDR);
+
+	/*
+	 * Configure valid bit on a fake value of bit 16. The ADC outputs
+	 * max of 2 bytes for voltage.
+	 */
+	writel(FIELD_PREP(EN7581_ADV_RD_VALID_POS, 16),
+	       priv->base + EN7581_TEMPADCVALIDMASK);
+
+	/*
+	 * AHB supports max 12 bytes for ADC voltage. Shift the read
+	 * value 4 bit to the right. Precision lost by this is minimal
+	 * in the order of half a °C and is acceptable in the context
+	 * of triggering interrupt in critical condition.
+	 */
+	writel(FIELD_PREP(EN7581_ADC_VOLTAGE_SHIFT, 4),
+	       priv->base + EN7581_TEMPADCVOLTAGESHIFT);
+
+	/* BUS clock is 300MHz counting unit is 3 * 68.64 * 256 = 52.715us */
+	writel(FIELD_PREP(EN7581_PERIOD_UNIT, 3),
+	       priv->base + EN7581_TEMPMONCTL1);
+
+	/*
+	 * filt interval is 1 * 52.715us = 52.715us,
+	 * sen interval is 379 * 52.715us = 19.97ms
+	 */
+	writel(FIELD_PREP(EN7581_FILT_INTERVAL, 1) |
+	       FIELD_PREP(EN7581_FILT_INTERVAL, 379),
+	       priv->base + EN7581_TEMPMONCTL2);
+
+	/* AHB poll is set to 146 * 68.64 = 10.02us */
+	writel(FIELD_PREP(EN7581_ADC_POLL_INTVL, 146),
+	       priv->base + EN7581_TEMPAHBPOLL);
+}
+
+static int airoha_thermal_probe(struct platform_device *pdev)
+{
+	struct thermal_zone_params tzp = { };
+	struct airoha_thermal_priv *priv;
+	struct device_node *chip_scu_np;
+	struct device *dev = &pdev->dev;
+	int irq, ret;
+
+	priv = devm_kzalloc(dev, sizeof(*priv), GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	priv->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(priv->base))
+		return PTR_ERR(priv->base);
+
+	chip_scu_np = of_parse_phandle(dev->of_node, "airoha,chip-scu", 0);
+	if (!chip_scu_np)
+		return -EINVAL;
+
+	priv->chip_scu = syscon_node_to_regmap(chip_scu_np);
+	if (IS_ERR(priv->chip_scu))
+		return PTR_ERR(priv->chip_scu);
+
+	of_address_to_resource(chip_scu_np, 0, &priv->scu_adc_res);
+	of_node_put(chip_scu_np);
+
+	irq = platform_get_irq(pdev, 0);
+	if (irq < 0)
+		return irq;
+
+	ret = devm_request_threaded_irq(&pdev->dev, irq, NULL,
+					airoha_thermal_irq, IRQF_ONESHOT,
+					pdev->name, (void *)priv);
+	if (ret) {
+		dev_err(dev, "Can't get interrupt working.\n");
+		return ret;
+	}
+
+	airoha_thermal_setup_monitor(priv);
+	airoha_thermal_setup_adc_val(dev, priv, &tzp);
+
+	/* register of thermal sensor and get info from DT */
+	priv->tz = devm_thermal_of_zone_register_with_params(dev, 0, priv,
+							     &thdev_ops,
+							     &tzp);
+	if (IS_ERR(priv->tz)) {
+		dev_err(dev, "register thermal zone sensor failed\n");
+		return PTR_ERR(priv->tz);
+	}
+
+	platform_set_drvdata(pdev, priv);
+
+	/* Enable LOW and HIGH interrupt */
+	writel(EN7581_HOFSINTEN0 | EN7581_LOFSINTEN0,
+	       priv->base + EN7581_TEMPMONINT);
+
+	return 0;
+}
+
+static const struct of_device_id airoha_thermal_match[] = {
+	{ .compatible = "airoha,en7581-thermal" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, airoha_thermal_match);
+
+static struct platform_driver airoha_thermal_driver = {
+	.driver = {
+		.name = "airoha-thermal",
+		.of_match_table = airoha_thermal_match,
+	},
+	.probe = airoha_thermal_probe,
+};
+
+module_platform_driver(airoha_thermal_driver);
+
+MODULE_AUTHOR("Christian Marangi <ansuelsmth@gmail.com>");
+MODULE_DESCRIPTION("Airoha thermal driver");
+MODULE_LICENSE("GPL");
