From 7dfed4b67bd6ba8c33caf90c01821b67cf3260dd Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <emil.renner.berthing@canonical.com>
Date: Sat, 25 Mar 2023 23:04:31 +0100
Subject: [PATCH 1007/1024] clk: starfive: jh7100: Add CLK_SET_RATE_PARENT to
 gmac_tx

This is needed by the dwmac-starfive ethernet driver to set the clock
for 1000, 100 and 10 Mbps links properly.

Signed-off-by: Emil Renner Berthing <emil.renner.berthing@canonical.com>
---
 drivers/clk/starfive/clk-starfive-jh7100.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/clk/starfive/clk-starfive-jh7100.c
+++ b/drivers/clk/starfive/clk-starfive-jh7100.c
@@ -200,7 +200,7 @@ static const struct jh71x0_clk_data jh71
 	JH71X0_GDIV(JH7100_CLK_GMAC_GTX, "gmac_gtxclk", 0, 255, JH7100_CLK_GMAC_ROOT_DIV),
 	JH71X0_GDIV(JH7100_CLK_GMAC_RMII_TX, "gmac_rmii_txclk", 0, 8, JH7100_CLK_GMAC_RMII_REF),
 	JH71X0_GDIV(JH7100_CLK_GMAC_RMII_RX, "gmac_rmii_rxclk", 0, 8, JH7100_CLK_GMAC_RMII_REF),
-	JH71X0__MUX(JH7100_CLK_GMAC_TX, "gmac_tx", 0, 3,
+	JH71X0__MUX(JH7100_CLK_GMAC_TX, "gmac_tx", CLK_SET_RATE_PARENT | CLK_SET_RATE_NO_REPARENT, 3,
 		    JH7100_CLK_GMAC_GTX,
 		    JH7100_CLK_GMAC_TX_INV,
 		    JH7100_CLK_GMAC_RMII_TX),
