config global
#	option uci_enabled '1'

config network
	# Logical network dependency, fully tracked, fwknopd gets restarted when
	# necessary. Specifying network takes precedence over config.PCAP_INTF
#	option network 'wan'

config access
	option SOURCE 'ANY'
	option HMAC_KEY 'CHANGEME'
	option KEY 'CHANGEME'

config config
	# Alternative direct physical interface definition, but untracked - you
	# are on your own to correctly start/stop the service when needed
#	option PCAP_INTF 'eth0'
