From: =?UTF-8?q?Rog=C3=A9rio=20Brito?= <rbrito@ime.usp.br>
Date: Thu, 24 Oct 2013 01:11:21 -0200
Subject: Adjust types for printing

Try to address the issues of a given integral type having different sizes
in 32 and 64-bit architectures.
---
 fsck_hfs.tproj/dfalib/SControl.c   | 2 +-
 fsck_hfs.tproj/dfalib/hfs_endian.c | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/fsck_hfs.tproj/dfalib/SControl.c
+++ b/fsck_hfs.tproj/dfalib/SControl.c
@@ -776,7 +776,7 @@ static int ScavSetUp( SGlob *GPtr)
 		pointer = (ScavStaticStructures *) AllocateClearMemory( sizeof(ScavStaticStructures) );
 		if ( pointer == nil ) {
 			if ( GPtr->logLevel >= kDebugLog ) {
-				printf( "\t error %d - could not allocate %ld bytes of memory \n",
+				printf( "\t error %d - could not allocate %i bytes of memory \n",
 					R_NoMem, sizeof(ScavStaticStructures) );
 			}
 			return( R_NoMem );
--- a/fsck_hfs.tproj/dfalib/hfs_endian.c
+++ b/fsck_hfs.tproj/dfalib/hfs_endian.c
@@ -563,7 +563,7 @@ hfs_swap_HFSPlusBTInternalNode (
             /* Make sure name length is consistent with key length */
             if (keyLength < sizeof(srcKey->parentID) + sizeof(srcKey->nodeName.length) +
                 srcKey->nodeName.length*sizeof(srcKey->nodeName.unicode[0])) {
-				if (debug) printf("hfs_swap_HFSPlusBTInternalNode: catalog record #%d keyLength=%d expected=%lu\n",
+				if (debug) printf("hfs_swap_HFSPlusBTInternalNode: catalog record #%d keyLength=%d expected=%i\n",
 					srcDesc->numRecords-i, keyLength, sizeof(srcKey->parentID) + sizeof(srcKey->nodeName.length) +
                     srcKey->nodeName.length*sizeof(srcKey->nodeName.unicode[0]));
 				WriteError(fcb->fcbVolume->vcbGPtr, E_KeyLen, fcb->fcbFileID, src->blockNum);
