// Boot BIF example for wolfBoot with signed Hello World
// Note: "partition_owner=uboot" prevents partition from being loaded to RAM
the_ROM_image:
{
	[bootloader, destination_cpu=a53-0] zynqmp_fsbl.elf
	[destination_cpu=pmu] pmufw.elf
	[destination_device=pl] system.bit
	[destination_cpu=a53-0, exception_level=el-3, trustzone] bl31.elf
	[destination_cpu=a53-0, exception_level=el-1] wolfboot.elf
	[destination_cpu=a53-0, partition_owner=uboot, offset=0x800000] helloworld_v1_signed.bin
}
