<config configName="default" projectName="test-usb-updater.same51" configVersion="1.1" device="ATSAME51J20A" deviceLibraryClass="com.microchip.mcc.harmony.Harmony3Library" coreVersion="5.7.0">
   <usedPackages class="java.util.ArrayList"/>
   <usedClasses class="java.util.TreeMap">
      <entry>
         <string>cmsis</string>
         <string>class com.microchip.mcc.harmony.HarmonyModule</string>
      </entry>
      <entry>
         <string>core</string>
         <string>class com.microchip.mcc.harmony.HarmonyModule</string>
      </entry>
      <entry>
         <string>dfp</string>
         <string>class com.microchip.mcc.harmony.HarmonyModule</string>
      </entry>
      <entry>
         <string>evsys</string>
         <string>class com.microchip.mcc.harmony.HarmonyModule</string>
      </entry>
      <entry>
         <string>nvmctrl</string>
         <string>class com.microchip.mcc.harmony.HarmonyModule</string>
      </entry>
      <entry>
         <string>sercom5</string>
         <string>class com.microchip.mcc.harmony.HarmonyModule</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.harmony.Harmony3Library" version="1.5.1"/>
   </usedLibraries>
   <tokenMap class="java.util.TreeMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="cmsis" name="#&amp;__MCC_Group_Parrent_id"/>
         <value>__ROOTVIEW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="!@#harmonyUserData"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;UserData&gt;
  &lt;UserData dnOrder=&quot;0&quot;&gt;
    &lt;GraphSettings canvasHeight=&quot;315&quot; canvasWidth=&quot;641&quot; dnOrder=&quot;0&quot;/&gt;
    &lt;PowerProfiles dnOrder=&quot;1&quot;&gt;
      &lt;Profile dnOrder=&quot;0&quot; id=&quot;profile0&quot; name=&quot;Main&quot;/&gt;
    &lt;/PowerProfiles&gt;
    &lt;ComponentGraph dnOrder=&quot;2&quot; id=&quot;__ROOTVIEW&quot;&gt;
      &lt;ElementPositions dnOrder=&quot;0&quot;&gt;
        &lt;ElementPosition dnOrder=&quot;0&quot; id=&quot;cmsis&quot; x=&quot;330&quot; y=&quot;60&quot;/&gt;
        &lt;ElementPosition dnOrder=&quot;1&quot; id=&quot;core&quot; x=&quot;560&quot; y=&quot;20&quot;/&gt;
        &lt;ElementPosition dnOrder=&quot;2&quot; id=&quot;dfp&quot; x=&quot;340&quot; y=&quot;20&quot;/&gt;
        &lt;ElementPosition dnOrder=&quot;3&quot; id=&quot;evsys&quot; x=&quot;180&quot; y=&quot;20&quot;/&gt;
        &lt;ElementPosition dnOrder=&quot;4&quot; id=&quot;nvmctrl&quot; x=&quot;20&quot; y=&quot;20&quot;/&gt;
        &lt;ElementPosition dnOrder=&quot;5&quot; id=&quot;sercom5&quot; x=&quot;179&quot; y=&quot;154&quot;/&gt;
      &lt;/ElementPositions&gt;
    &lt;/ComponentGraph&gt;
  &lt;/UserData&gt;
&lt;/UserData&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="#&amp;__MCC_Group_Parrent_id"/>
         <value>__ROOTVIEW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="GCLK_ID_35_CHEN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;GCLK_ID_35_CHEN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="GCLK_ID_35_FREQ"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;GCLK_ID_35_FREQ&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;60000000&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="MCLK_APBD_INITIAL_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;MCLK_APBD_INITIAL_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;0x2&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_66_0_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_66_0_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
      &lt;User dnOrder=&quot;1&quot; value=&quot;false&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_66_0_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_66_0_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
      &lt;User dnOrder=&quot;1&quot; value=&quot;SERCOM5_0_Handler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_66_0_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_66_0_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_67_0_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_67_0_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
      &lt;User dnOrder=&quot;1&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_67_0_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_67_0_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_67_0_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_67_0_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_68_0_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_68_0_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
      &lt;User dnOrder=&quot;1&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_68_0_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_68_0_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_68_0_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_68_0_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_69_0_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_69_0_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
      &lt;User dnOrder=&quot;1&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_69_0_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_69_0_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="NVIC_69_0_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;NVIC_69_0_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PIN_39_FUNCTION_TYPE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PIN_39_FUNCTION_TYPE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;SERCOM5_PAD0&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PIN_39_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PIN_39_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PIN_39_PERIPHERAL_FUNCTION"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PIN_39_PERIPHERAL_FUNCTION&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;C&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PIN_40_FUNCTION_TYPE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PIN_40_FUNCTION_TYPE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;SERCOM5_PAD1&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PIN_40_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PIN_40_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PIN_40_PERIPHERAL_FUNCTION"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PIN_40_PERIPHERAL_FUNCTION&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;C&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PAD_16"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PAD_16&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;PB16&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PAD_17"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PAD_17&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;PB17&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PINCFG16"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PINCFG16&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;0x1&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PINCFG17"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PINCFG17&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;0x1&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PIN_16_USED"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PIN_16_USED&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PIN_17_USED"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PIN_17_USED&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="PORT_GROUP_1_PMUX8"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;PORT_GROUP_1_PMUX8&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;0x22&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_0_INTERRUPT_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_0_INTERRUPT_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_0_INTERRUPT_ENABLE_UPDATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_0_INTERRUPT_ENABLE_UPDATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_0_INTERRUPT_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_0_INTERRUPT_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_0_INTERRUPT_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_0_INTERRUPT_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_1_INTERRUPT_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_1_INTERRUPT_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_1_INTERRUPT_ENABLE_UPDATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_1_INTERRUPT_ENABLE_UPDATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;false&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_1_INTERRUPT_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_1_INTERRUPT_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_1_INTERRUPT_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_1_INTERRUPT_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_2_INTERRUPT_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_2_INTERRUPT_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_2_INTERRUPT_ENABLE_UPDATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_2_INTERRUPT_ENABLE_UPDATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;false&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_2_INTERRUPT_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_2_INTERRUPT_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_2_INTERRUPT_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_2_INTERRUPT_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_CORE_CLOCK_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_CORE_CLOCK_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_CORE_CLOCK_FREQUENCY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_CORE_CLOCK_FREQUENCY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;60000000&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_OTHER_INTERRUPT_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_OTHER_INTERRUPT_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_OTHER_INTERRUPT_ENABLE_UPDATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_OTHER_INTERRUPT_ENABLE_UPDATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;core&quot; value=&quot;false&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_OTHER_INTERRUPT_HANDLER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_OTHER_INTERRUPT_HANDLER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;SERCOM5_USART_InterruptHandler&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="core" name="SERCOM5_OTHER_INTERRUPT_HANDLER_LOCK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;core&gt;
  &lt;core dnOrder=&quot;0&quot; id=&quot;SERCOM5_OTHER_INTERRUPT_HANDLER_LOCK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/core&gt;
&lt;/core&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="dfp" name="#&amp;__MCC_Group_Parrent_id"/>
         <value>__ROOTVIEW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="evsys" name="#&amp;__MCC_Group_Parrent_id"/>
         <value>__ROOTVIEW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="nvmctrl" name="#&amp;__MCC_Group_Parrent_id"/>
         <value>__ROOTVIEW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="#&amp;__MCC_Group_Parrent_id"/>
         <value>__ROOTVIEW</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CM_ADDR_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CM_ADDR_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CM_BAUD"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CM_BAUD&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;255&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CM_BAUD_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CM_BAUD_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CM_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CM_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CM_TRISE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CM_TRISE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_INTENSET_ERROR"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_INTENSET_ERROR&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_INTERRUPT_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_INTERRUPT_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_LOWTOUT_ERROR_SUPPORT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_LOWTOUT_ERROR_SUPPORT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_LOWTOUT_SUPPORT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_LOWTOUT_SUPPORT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_PLIB_API_PREFIX"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_PLIB_API_PREFIX&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_RUNSTDBY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_RUNSTDBY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SCLSM"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SCLSM&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SDAHOLD_TIME"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SDAHOLD_TIME&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SDASETUP_MAX_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SDASETUP_MAX_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SDASETUP_TIME_NS"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SDASETUP_TIME_NS&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SDASETUP_TIME_REG_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SDASETUP_TIME_REG_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SDASETUP_TIME_SUPPORT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SDASETUP_TIME_SUPPORT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SEXTTOEN_SUPPORT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SEXTTOEN_SUPPORT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SEXTTOOUT_ERROR_SUPPORT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SEXTTOOUT_ERROR_SUPPORT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SLAVE_ADDDRESS"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SLAVE_ADDDRESS&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_SMEN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_SMEN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2CS_TENBITEN_SUPPORT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2CS_TENBITEN_SUPPORT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_ADDR_TENBITEN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_ADDR_TENBITEN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_CLOCK_SPEED"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_CLOCK_SPEED&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_CLOCK_SPEED_HZ"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_CLOCK_SPEED_HZ&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_INTERRUPT_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_INTERRUPT_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_MASTER_CODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_MASTER_CODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_PLIB_API_PREFIX"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_PLIB_API_PREFIX&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_RUNSTDBY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_RUNSTDBY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_SCLSM"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_SCLSM&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="I2C_SDAHOLD_TIME"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;I2C_SDAHOLD_TIME&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="RECEIVE_DATA_REGISTER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;RECEIVE_DATA_REGISTER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SERCOM_INSTANCE_NAME"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SERCOM_INSTANCE_NAME&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SERCOM_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SERCOM_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SERCOM_SYNCBUSY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SERCOM_SYNCBUSY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SERCOM_USART_HEADER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SERCOM_USART_HEADER&quot;&gt;
    &lt;Attributes dnOrder=&quot;0&quot;&gt;
      &lt;String dnOrder=&quot;0&quot; id=&quot;source&quot;&gt;
        &lt;Value dnOrder=&quot;0&quot;&gt;../peripheral/sercom_u2201/templates/plib_sercom_usart.h.ftl&lt;/Value&gt;
      &lt;/String&gt;
    &lt;/Attributes&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SERCOM_USART_SOURCE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SERCOM_USART_SOURCE&quot;&gt;
    &lt;Attributes dnOrder=&quot;0&quot;&gt;
      &lt;String dnOrder=&quot;0&quot; id=&quot;source&quot;&gt;
        &lt;Value dnOrder=&quot;0&quot;&gt;../peripheral/sercom_u2201/templates/plib_sercom_usart.c.ftl&lt;/Value&gt;
      &lt;/String&gt;
    &lt;/Attributes&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_BUSY_PIN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_BUSY_PIN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_BUSY_PIN_LOGIC_LEVEL"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_BUSY_PIN_LOGIC_LEVEL&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_CHARSIZE_BITS"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_CHARSIZE_BITS&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_CLOCK_PHASE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_CLOCK_PHASE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_CLOCK_POLARITY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_CLOCK_POLARITY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_DATA_ORDER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_DATA_ORDER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_DATA_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_DATA_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_DIPO"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_DIPO&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_DOPO"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_DOPO&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_INTENSET_ERROR"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_INTENSET_ERROR&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_INTERRUPT_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_INTERRUPT_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_RUNSTDBY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_RUNSTDBY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_RX_BUFFER_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_RX_BUFFER_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_SSDE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_SSDE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_TX_BUFFER_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_TX_BUFFER_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPIS_USE_BUSY_PIN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPIS_USE_BUSY_PIN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_BAUD_RATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_BAUD_RATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_BAUD_REG_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_BAUD_REG_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;29&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CHARSIZE_BITS"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CHARSIZE_BITS&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CHARSIZE_BITS_8_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CHARSIZE_BITS_8_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CHARSIZE_BITS_9_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CHARSIZE_BITS_9_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CLOCK_PHASE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CLOCK_PHASE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CLOCK_PHASE_LEADING_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CLOCK_PHASE_LEADING_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CLOCK_PHASE_TRAILING_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CLOCK_PHASE_TRAILING_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CLOCK_POLARITY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CLOCK_POLARITY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CLOCK_POLARITY_HIGH_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CLOCK_POLARITY_HIGH_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_CLOCK_POLARITY_LOW_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_CLOCK_POLARITY_LOW_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_DATA_ORDER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_DATA_ORDER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_DIPO"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_DIPO&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_DOPO"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_DOPO&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_INTENSET_ERROR"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_INTENSET_ERROR&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_INTERRUPT_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_INTERRUPT_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_MSSEN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_MSSEN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_PLIB_API_PREFIX"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_PLIB_API_PREFIX&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_RECIEVER_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_RECIEVER_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_RUNSTDBY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_RUNSTDBY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="SPI_STATUS_OVERRUN_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;SPI_STATUS_OVERRUN_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="TRANSMIT_DATA_REGISTER"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;TRANSMIT_DATA_REGISTER&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_BAUD_RATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_BAUD_RATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_BAUD_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_BAUD_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;63522&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_CHARSIZE_BITS"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_CHARSIZE_BITS&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_CTRLC_GTIME"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_CTRLC_GTIME&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_DATA_5_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_DATA_5_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_DATA_6_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_DATA_6_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_DATA_7_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_DATA_7_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_DATA_8_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_DATA_8_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_DATA_9_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_DATA_9_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_DATA_BITS"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_DATA_BITS&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_FLOW_CONTROL"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_FLOW_CONTROL&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_FORM"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_FORM&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_FRAMING_ERROR_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_FRAMING_ERROR_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_INTENSET_ERROR"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_INTENSET_ERROR&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_INTERRUPT_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_INTERRUPT_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_INTERRUPT_MODE_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_INTERRUPT_MODE_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_LIN_MASTER_BREAK_LEN"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_LIN_MASTER_BREAK_LEN&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_LIN_MASTER_HDRDLY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_LIN_MASTER_HDRDLY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_LIN_MASTER_SUPPORTED"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_LIN_MASTER_SUPPORTED&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;true&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_OPERATING_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_OPERATING_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;1&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_OVERRUN_ERROR_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_OVERRUN_ERROR_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_PARITY_ERROR_VALUE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_PARITY_ERROR_VALUE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_PARITY_EVEN_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_PARITY_EVEN_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_PARITY_MODE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_PARITY_MODE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_PARITY_NONE_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_PARITY_NONE_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_PARITY_ODD_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_PARITY_ODD_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_PLIB_API_PREFIX"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_PLIB_API_PREFIX&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RING_BUFFER_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RING_BUFFER_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RING_BUFFER_MODE_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RING_BUFFER_MODE_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;false&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RS485"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RS485&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RUNSTDBY"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RUNSTDBY&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;User dnOrder=&quot;0&quot; value=&quot;false&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RXPO"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RXPO&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RX_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RX_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_RX_RING_BUFFER_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_RX_RING_BUFFER_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_SAMPLE_COUNT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_SAMPLE_COUNT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;16&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_SAMPLE_RATE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_SAMPLE_RATE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;&gt;
      &lt;Dynamic dnOrder=&quot;0&quot; id=&quot;sercom5&quot; value=&quot;0&quot;/&gt;
    &lt;/Values&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_SFDE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_SFDE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_STOP_1_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_STOP_1_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_STOP_2_BIT_MASK"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_STOP_2_BIT_MASK&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_STOP_BIT"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_STOP_BIT&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_TXPO"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_TXPO&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_TX_ENABLE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_TX_ENABLE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="sercom5" name="USART_TX_RING_BUFFER_SIZE"/>
         <value>&lt;?xml version=&quot;1.0&quot; encoding=&quot;UTF-8&quot;?&gt;&lt;sercom5&gt;
  &lt;sercom5 dnOrder=&quot;0&quot; id=&quot;USART_TX_RING_BUFFER_SIZE&quot;&gt;
    &lt;Values dnOrder=&quot;0&quot;/&gt;
  &lt;/sercom5&gt;
&lt;/sercom5&gt;
</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.TreeMap">
      <entry>
         <file>../src/config/default/ATSAME51J20A.ld</file>
         <hash>15cc39143f19337d981ec510fb70d42c944cd8b2cf96c6fe85f9c053341dfae2</hash>
      </entry>
      <entry>
         <file>../src/config/default/definitions.h</file>
         <hash>a3e220bb8905f3e52cca32c4ac9a814d3e58c25ae9f3bcc5b3a1e9d13f117a70</hash>
      </entry>
      <entry>
         <file>../src/config/default/device.h</file>
         <hash>5ef6927cc338505efe55c8d90bcf721643a2210567cd529c1d26195b8a96f17f</hash>
      </entry>
      <entry>
         <file>../src/config/default/device_cache.h</file>
         <hash>e2914501b361bbc93a56d6915b1bf4fac00277e61f31fdee87a587bc15dea5b6</hash>
      </entry>
      <entry>
         <file>../src/config/default/device_vectors.h</file>
         <hash>73940897ea4570f75fde55f65cc755757d1989db12e039b9960b0de07853cb45</hash>
      </entry>
      <entry>
         <file>../src/config/default/exceptions.c</file>
         <hash>1fd383302c4cdf1cc6a804aa03b8abe8c1e5e5e9ea3450438c34dcea441e6b34</hash>
      </entry>
      <entry>
         <file>../src/config/default/initialization.c</file>
         <hash>43a3d0f21ead5914e46d18c31e1285403cc308a18c26e95ee99829d848e38bd6</hash>
      </entry>
      <entry>
         <file>../src/config/default/interrupts.c</file>
         <hash>1fd61b9edde4a66bd7d8fe7c21294439bd6433e32f296b2766d72ef847855783</hash>
      </entry>
      <entry>
         <file>../src/config/default/interrupts.h</file>
         <hash>9e8b7e9f6877331da7a486c6e8de42ba7caa87ffdb0ca3b903fc3c62c0ee0233</hash>
      </entry>
      <entry>
         <file>../src/config/default/libc_syscalls.c</file>
         <hash>88bb2e34c939601b5b7ad076556e3ee0fcedf388436b8cddb6d6fd3e9d07472f</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/clock/plib_clock.c</file>
         <hash>bc8c16c339d428ea109c1b74d34e7cd1e82ad485352b62b263dbf4fee5b46d82</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/clock/plib_clock.h</file>
         <hash>59322a99314cb17c6b595d51d18769582e61189140188aa053acfdc671487f21</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/cmcc/plib_cmcc.c</file>
         <hash>3b03e762c5515130718e7694736be6c25984ff8078c84d21a3fb9eba54f68e5d</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/cmcc/plib_cmcc.h</file>
         <hash>89b940242bfa0ecdba3ac53666c5996e25fab712227d37d2d6881c8a86b5f497</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/evsys/plib_evsys.c</file>
         <hash>b2e1a8004049e687fc5544133f3346f743ced50cdaf860c8e3c7f58df3cc163f</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/evsys/plib_evsys.h</file>
         <hash>f7d08eb8162f271ce1db384c082586a6624e506aa7f502c64c4ab5a1aadac47d</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/nvic/plib_nvic.c</file>
         <hash>27a04bb02dc989f8ddf9d5b252e769f1d4533b21f887968b63bd71c06c0d7316</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/nvic/plib_nvic.h</file>
         <hash>81e813a093101d546799e00723cbf7245e2d18471fa51c8d130c5809cecca03e</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/nvmctrl/plib_nvmctrl.c</file>
         <hash>1a6bdac00590cbec796a13351597c695bc1d962a95641bdb573d1bf0dc38b2d8</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/nvmctrl/plib_nvmctrl.h</file>
         <hash>fd7749dc74a885efd7c593394454abc74afc7cf184123f0315425a3600c26ac5</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/port/plib_port.c</file>
         <hash>589d2d648ef2b6147f7ac519986c4194148d612a9cc977ef81ad2048ec9a737c</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/port/plib_port.h</file>
         <hash>e960c88b8ed75f85e9c8997353bb7de730dd73d0dd2590130b50a245047d8949</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/sercom/usart/plib_sercom5_usart.c</file>
         <hash>5558b71299b1f1fc8d085d2419cfb2cf0753b2e2516c76fa4c3883f3fe7eb2e5</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/sercom/usart/plib_sercom5_usart.h</file>
         <hash>c1b506966a99e2e2c73d0a415917a028ce593d827e324d6035e5d5dbf135115f</hash>
      </entry>
      <entry>
         <file>../src/config/default/peripheral/sercom/usart/plib_sercom_usart_common.h</file>
         <hash>f19dafabe0928d60dd83d7e19f35889f200e3fbadff09e2f42523d320acf780a</hash>
      </entry>
      <entry>
         <file>../src/config/default/pin_configurations.csv</file>
         <hash>16a4a6fb78bf3f21aa3966903bc0298f705b763502f94f80d8a9b5890fff9a48</hash>
      </entry>
      <entry>
         <file>../src/config/default/startup_xc32.c</file>
         <hash>f374b97d65f92553f1b75d8c9239b8b0f8581c710f78ea47b02c7f6fa6f74c74</hash>
      </entry>
      <entry>
         <file>../src/config/default/stdio/xc32_monitor.c</file>
         <hash>858f8710d4287200a5ee7f3b3ad7c24f505aed9c05c16956ab0ff9f7bb162a6a</hash>
      </entry>
      <entry>
         <file>../src/config/default/toolchain_specifics.h</file>
         <hash>6fc0551b0fa3362678b3d7a227386fafa343140d31e4da3ad4af972e61cd0acb</hash>
      </entry>
      <entry>
         <file>../src/main.c</file>
         <hash>d3c233d419e6304bfacbafc18cc68c0f5c26e365f23b20ea40ccfac458f664c5</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/ac.h</file>
         <hash>3c654199445119481841c9673fa7616d050f5c83a9dfe626287e55d077a05439</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/adc.h</file>
         <hash>40c635359e8eb7b5c0f457a98758c69556415279ac6e7227d20d18dc27b5d5bd</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/aes.h</file>
         <hash>330b0c7b3473018c47f25a557c7110222a7b0e070e01a355c8559b9844f13b16</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/can.h</file>
         <hash>615dbf905d4a45aa3a7803794d00661df310cde437ed94f7d5bc8e205a2d0d0c</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/ccl.h</file>
         <hash>23babd444ac6b2ee91f67b98d8f0f9209bab96aa57d88d0d0d16e2b50e919126</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/cmcc.h</file>
         <hash>4b3e61a49ccf4dfa0325e5fb6349f35230b96e27ecdc907ae3d6901155d0b0fe</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/dac.h</file>
         <hash>76d210acf5a15a1be9833feb465a07c3b8465595830a3c008dee79d896787973</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/dmac.h</file>
         <hash>4b0176f10816bff2775ccac6b1a6c7dd6b0e10c16399a84bd787b5d0c94c285d</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/dsu.h</file>
         <hash>f29f83b0bb5829d43a29ec29e66556fc8e6dd417bf8c20022a611bab1a3c5823</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/eic.h</file>
         <hash>2e19b9a1f44567da7f09710746824495e0c2ea389fed92ab22460f43da5c1718</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/evsys.h</file>
         <hash>d44a0b5b6b6787dba61ce9f02082c63efd1a36c9d9354843a2aee02697532c65</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/freqm.h</file>
         <hash>275513ff8cda33e2896fb114b6f9b1d2679a22756c6d212b6d1ecf620b5a3750</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/fuses.h</file>
         <hash>340ba40f72c13340132c5dd060ef5a7dff423b38313595364b92bbf95f12757c</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/gclk.h</file>
         <hash>26926e2483df5de1da579caa924a23027a51941e4fdcd070a4d333bd6f16f121</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/hmatrixb.h</file>
         <hash>2d469ff5c0faef3e13a5a441395babb7f94cfe556ef5a553a01e214c5bc45705</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/i2s.h</file>
         <hash>cb1cad95694f5a301efa483741a19095cccb332aa9d773205a7d16721f4a8339</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/icm.h</file>
         <hash>c13cc80fc05733bb2544714b8d37fb1030023fd51b325b7c85e1e434c5fd5e0d</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/mclk.h</file>
         <hash>44413a208e2f0f407f236cd262949ed8c9b527b8461bac4d532c5f4338e8c54a</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/nvmctrl.h</file>
         <hash>519bd8b81f3df727a34f3a9c81ad96eca25c6b4e7df166e25113291f50062415</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/osc32kctrl.h</file>
         <hash>8babf9629ac21b2cff66fc30dad2ff31f64a5b2228a1fef275e8e146d66ed85d</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/oscctrl.h</file>
         <hash>c51b1aed31d3e7880a01e22dbff241ad3ca50930aeec25db054ed27430121251</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/pac.h</file>
         <hash>dada7b6dc528c64369ef4ed0acbc541601b651cb4fbd8edd5b2eb86e2bd84640</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/pcc.h</file>
         <hash>2736f552a080e6bdfcaaf1f2a30e8ee65dc934c34c2789a7ac338e620c095070</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/pdec.h</file>
         <hash>dbea79497d409b29fda82f081c8157d55b2d11e7337a4299dca8bde16d8143f4</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/pm.h</file>
         <hash>35b6594a249d8ea14fa2fe73ee4f9b1fcd73a87ae1627e27bdf99a6c0bcecdd6</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/port.h</file>
         <hash>f1ee8cd8dcb2f3fde2a650e76b7d7f7c5f124d0b5bb2cd9defa51c5d479dcfd7</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/pukcc.h</file>
         <hash>02edb60314483cee7eb86e97af5eacbdb14fb68a77ec810c88742ebf123d3008</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/qspi.h</file>
         <hash>320c3fe9bf885a689631c05bf588b0fe00f644c72b9cb4f8e443628165926be4</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/ramecc.h</file>
         <hash>c0e2cfc641f9b1450f4aff22d76a2e654cb196b6d1315d189db597ff39c2d893</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/rstc.h</file>
         <hash>425f9b775eb79abefdf1f2a09a9b2a39af45383f9a1065577ca4af580ead50c4</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/rtc.h</file>
         <hash>6850767b6f183fd4ff5a672c62b5b4c3b6e6b4ce66772db71457bafc7c9b6995</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/sdhc.h</file>
         <hash>9c5c0da9a2c74c7a560fd5218ac4054a5b66f35724eeaf5060f0daadd0dc7761</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/sercom.h</file>
         <hash>9cfd58850bdbe5f52b6fbc8a6b5b5e999a0dde485454e7551fb17ef1c124fa94</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/supc.h</file>
         <hash>411f832c5788198d4cd12258d78b67c54084b0a594bdc24a5025160b0331c36f</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/tc.h</file>
         <hash>c94e8a55afafa40a1730a655f23eb06a6793dcb4885f40fd0c96205afac6c24f</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/tcc.h</file>
         <hash>32fa9a257fc55388a157eb555d265e28be86e50f5067bdb6457c31d12bc93179</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/trng.h</file>
         <hash>06ba2ceb1c5711e86292cea5d1905f84e9898272d2525adff359bb725e1ec3f9</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/usb.h</file>
         <hash>1428aee3c7e6b6c46411db4ee6371ff23c638ac2167f3c00ebfc005fff32ccfe</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/component/wdt.h</file>
         <hash>2b810e4d10c04da4fa6666404a906977754fadbb07fdd94a27c0e812399eaed7</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/ac.h</file>
         <hash>cf8bccadca5bd7bb22ebbb82ca6b2d0a911861a0830fc086271f5dfe3845cd6f</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/adc0.h</file>
         <hash>cae698d90e4c21306151dff1dfedc3ca6cf46c05bb8a6cdc5a99cb18e7de07aa</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/adc1.h</file>
         <hash>a40b86bca6b1a2689a49f14a6ae1002097e2c5e5b665024a54c1d35e22abd10c</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/aes.h</file>
         <hash>9d63c362f34006299462514e958c7ae4eff54fa34073bffef377fc99e4daf873</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/can0.h</file>
         <hash>08991dcd49141a18f5e3ccc2e8c7a93e9fda7f3872a9abf3253909c4bbd542e4</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/can1.h</file>
         <hash>f02bc9abf7f8c1bdc2d8f46d49b368f6108ef1f6e6703193406445f4fddd801e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/ccl.h</file>
         <hash>af381c20215324c33792c1522f02df6787ebd271ffdc5b9510c6f2c25674ff22</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/cmcc.h</file>
         <hash>c1c3bfcd8afc805c7bd3687c01b61e36f857fae9b35f62fe32800d3a022d65d9</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/dac.h</file>
         <hash>6bb0cb75ad81eb2af278be9dbaa47de0a71a2f7fede6999b7357977716a00346</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/dmac.h</file>
         <hash>7f1b3b22396404b2b3b29519d18163e06d7832a55e7267ed12234b70b4bf3ac8</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/dsu.h</file>
         <hash>ecf9aa94c178309ee5ff34774ea02c229596fd831559c837ecb4cffa3d855ef9</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/eic.h</file>
         <hash>82e4df0e59cb35e8f625507ccdfe79052cbd7e5164374e69b16ca332a92ddc32</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/evsys.h</file>
         <hash>d8fd9b40db458c6fd2c7c75c36950f10e91b39b4478d6cccfde4494c4c437dfb</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/freqm.h</file>
         <hash>23dc3da789a0fc659987dbd7f5853d88825f823b895711c79ae90b0705510197</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/fuses.h</file>
         <hash>ee648d899a8e97829f6b6c6cfa7a1f9ea196b7efc448480e8fed41fd679b429e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/gclk.h</file>
         <hash>a77e2d58a7958e96ed65639a352d185a3b1c305efb005ca22d2075cc575c4a09</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/hmatrix.h</file>
         <hash>4c00a55527fb9f54ecc8d5fd2ac13749fbd40c4dc878c763594a3f8a3e91e123</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/i2s.h</file>
         <hash>cbb23bdea8726d82803acc98f6e2151a89fb3aa16c2e41964bd955b19edb5d2b</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/icm.h</file>
         <hash>a8707627834d0dbdfb861bb44d5789665876b0cdfa961533a62cfe957957b68f</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/mclk.h</file>
         <hash>fcc32aec30f621e99ef7ed0a1b11c0478d2213c30a5f99df7b210eea7402b40e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/nvmctrl.h</file>
         <hash>79f841cd85017dce864c44cec0e9b623bb777bb7953dd3d950401ae507bcdc2e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/osc32kctrl.h</file>
         <hash>39b699dcd205a789714971a4d9e44f4c596cacc1f114acbc4bc9266f0a3b89c0</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/oscctrl.h</file>
         <hash>85fab1eebc94bb2f79ff54c6c0f28894d2e3b19adc661ceb4b33d201ad1047e3</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/pac.h</file>
         <hash>1af48f37cf4edeeae68ae435694667606a98ed679ebca28478ea23913574826e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/pcc.h</file>
         <hash>4e67b425da6c02c6d9c1de0119434da3aa3eeffed5739aebc84421b7c1e554a9</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/pdec.h</file>
         <hash>50866aab5cc4261f99750d110d343bb7c16d7db89747b0ad70a754c01da3bad8</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/pm.h</file>
         <hash>eefb8c1969dd3c6f68fa4e1041d8821acc7c864174a5c96bfbe35d768b8512e4</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/port.h</file>
         <hash>19736dce73ce13291fa4dc24ce6f6effb7d8c59909752ce0eedd66738a3ec2e6</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/qspi.h</file>
         <hash>8d25ad0cc93ecd727ea34792261d57dde7ff7ea1037c5fedc202c1b539496374</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/ramecc.h</file>
         <hash>b386ce590951347c4a00dae722b72aaf60352505d333d213066406ee2a19ca35</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/rstc.h</file>
         <hash>7b645b3c95e85b91dcaa285937200482d69f3912ad7be3fe111b7b1c858beb5a</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/rtc.h</file>
         <hash>5a08583905fa066ac8bbee3f34ec50e61b5876be0c2080a96e1ff7ed52cef866</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sdhc0.h</file>
         <hash>fd795d5cc7e5390e91fae90d9faaa4c93916943a1b1b9209906958c1631a08af</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom0.h</file>
         <hash>56de9750a91f40e891e90ebd2a94a972b26c3869b829f2765c7e6396b27d65fc</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom1.h</file>
         <hash>f99ef6978e99bae8edeb0f1b4dd3c01e85261c4eabcf6be3faa939aa481b2ac6</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom2.h</file>
         <hash>9ffc25b630889efc0a3f1b51a5107f83facd556dea4d57a6560254d1f4ec7e92</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom3.h</file>
         <hash>20637cdd91ed2bc7997cc056b28aa999a45853d43b41c0e12c82643711517774</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom4.h</file>
         <hash>435ee699b80f6b8a75097c2a0db75ff7d8edbe1f9007fb578f3efbc2deb346db</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom5.h</file>
         <hash>84d44cea0c3b1f4a2d530b61c438958be9f22cbac3cf0e66ac000ff6682261e1</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom6.h</file>
         <hash>20d49c52eaaad8d1bab8281311652fbf5d6a26e09fa90064931b9a3f186af2fb</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/sercom7.h</file>
         <hash>ef8dddcc272204308add1eee859b5cd96db394fcc573516f5d2c1e2f571b006f</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/supc.h</file>
         <hash>c712ec44db8c08f4ee1908257ff53b117d6404b13b253b4be443104e2947235e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc0.h</file>
         <hash>b926c72c60a5209f87f32a964953e5e18ed7156a1d0714b5bfc0964a3e4db4ad</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc1.h</file>
         <hash>59bb9638cf2d71cddc8006bcaa7b7d58ad51f3e1fb96b095345e10b9a4247e81</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc2.h</file>
         <hash>ea221f213bb9cb0b414df784fb7c6b1b77124c4dcc1f737a2029610a16c893c8</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc3.h</file>
         <hash>f7c91e3285c307ce3c6cf95908bbfe68463ee6ab8eeec972d26f2b85d6a2570e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc4.h</file>
         <hash>817a8896cb07727ea9ff7d533ea33c8e906676c28caf93f72090f9e1beb8aabc</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc5.h</file>
         <hash>4e52c5644bc17730eb7177697f1ca6ec5708db4a90e349926d47317cbc938c00</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc6.h</file>
         <hash>2bd39068e349d0347ae2e071add326502c244dd475856b02bc8d6c0a7aa9b5d5</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tc7.h</file>
         <hash>1ad42c8e1b17d3cdceddf87578a809f32424aadcef440977a93fca12d93c5f2e</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tcc0.h</file>
         <hash>35993e030cd19621a1fe05ba1fed264eaa2cd77c2476d619e24032665263cc63</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tcc1.h</file>
         <hash>f2dc0e5030d27eeacf2a74ade4bb7d7b5f2db413880f69b122a6eb0919a96af8</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tcc2.h</file>
         <hash>995085f7f1bef05c3aa92aad7fae05a2ef24a49611b432ef1bc39a4b5bdecea0</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tcc3.h</file>
         <hash>d853335dacd3275363c3a893f6f759b67ea9cda2d45c5e289df1d0dd04c0f312</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/tcc4.h</file>
         <hash>7f78b71763838a402bf50e197d913b422cb115b421243df1287eba926ce7d812</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/trng.h</file>
         <hash>c06a6922011ab2c282e886c72b6051a688829776cbf0786e746ef2d28f4accb0</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/usb.h</file>
         <hash>a8a9affbaabaa627aea80af70261ef21c21473e895df243fa1bf21a4f0feee1b</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/instance/wdt.h</file>
         <hash>0ee35e8dce59f82a8109aa51a481e6319e5e62a72424571fc92f49caefa33964</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/pio/same51j20a.h</file>
         <hash>92a8021af75873384445867c66105c2bdce6efe22262eeba31351d0de6b2cab3</hash>
      </entry>
      <entry>
         <file>../src/packs/ATSAME51J20A_DFP/same51j20a.h</file>
         <hash>08cbd43a3fbb4499ba422c6888a17a7ec0b804543dc116a41f1a448ce99b8551</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cachel1_armv7.h</file>
         <hash>6cdb5b324f2fd1bb5b2f47298ba6e6777e735d7cad3bb8d942cd36e2c6e65328</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_armcc.h</file>
         <hash>d074534d7106cec83474b3b0a897bd2553e1a8895ecbd54f4f4fb25928066eee</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_armclang.h</file>
         <hash>11b39b96ddc1125124762b3423a77b90dd40ea5b4582a3513830245046b24311</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_armclang_ltm.h</file>
         <hash>8621969ea669a1b230ff2125a760ef66d575c48cb45e9e457f768909abcbda46</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_compiler.h</file>
         <hash>869640702d811c4c63abb52206715c891a93fd03be954df5ad40d378355af3d6</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_gcc.h</file>
         <hash>3d4e265d0aa42f888385ccf073666e6ebb5ec9f834760b9da27c474e177f708d</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_iccarm.h</file>
         <hash>f28119adbc81fb0e3c957c9aebe8fb423ad93634e76ead3caa2b0818d2e123ae</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/cmsis_version.h</file>
         <hash>8cda7ac3ff6f0eb5e83c4fe613dd195151b24da54167f5c3c007e599a03f1edc</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/core_cm4.h</file>
         <hash>d59a9e3ed4cf43a3c74a2e48f344d41be2b6363ef9394ea2c551052fe553a6af</hash>
      </entry>
      <entry>
         <file>../src/packs/CMSIS/CMSIS/Core/Include/mpu_armv7.h</file>
         <hash>de1b5eb9ed566527b66dc06f4ecb6a43ab6800f7dac47e87c9cb42984dca41bb</hash>
      </entry>
   </generatedFileHashHistoryMap>
</config>