#
# Default main stack size
#
# This is typically way bigger than needed for stack size. See user_settings.h
#
CONFIG_ESP_MAIN_TASK_STACK_SIZE=55000

# Legacy stack size for older ESP-IDF versions
CONFIG_MAIN_TASK_STACK_SIZE=55000

#
# Compiler options
#
CONFIG_COMPILER_OPTIMIZATION_DEFAULT=y
CONFIG_COMPILER_OPTIMIZATION_ASSERTIONS_ENABLE=y
CONFIG_COMPILER_OPTIMIZATION_ASSERTION_LEVEL=2
CONFIG_COMPILER_HIDE_PATHS_MACROS=y
CONFIG_COMPILER_STACK_CHECK_MODE_NORM=y
CONFIG_COMPILER_STACK_CHECK=y

# minimum C3 chip revision known to work is 2.
# rev 0 and 1 not available for testing.
# all revisions expected to work.
CONFIG_ESP32C3_REV_MIN_0=
CONFIG_ESP32C3_REV_MIN_1=
CONFIG_ESP32C3_REV_MIN_2=y
CONFIG_ESP32C3_REV_MIN_3=

#
# Partition Table
#
CONFIG_PARTITION_TABLE_SINGLE_APP_LARGE=y
CONFIG_PARTITION_TABLE_CUSTOM_FILENAME="partitions.csv"
CONFIG_PARTITION_TABLE_FILENAME="partitions_singleapp_large.csv"
CONFIG_PARTITION_TABLE_OFFSET=0x8000
CONFIG_PARTITION_TABLE_MD5=y
# end of Partition Table
