/* wifi_connect.c
 *
 * Copyright (C) 2006-2023 wolfSSL Inc.
 *
 * This file is part of wolfSSL.
 *
 * wolfSSL is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation; either version 2 of the License, or
 * (at your option) any later version.
 *
 * wolfSSL is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 *
 * You should have received a copy of the GNU General Public License
 * along with this program; if not, write to the Free Software
 * Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA 02110-1335, USA
 */
/*ESP specific */
#include "freertos/FreeRTOS.h"
#include "freertos/task.h"
#include "freertos/event_groups.h"
#include "wifi_connect.h"
#include "lwip/sockets.h"
#include "lwip/netdb.h"
#include "lwip/apps/sntp.h"
#include "nvs_flash.h"

/* wolfSSL */
#include <wolfssl/wolfcrypt/settings.h>
#include <user_settings.h>
#include <wolfssl/version.h>
#ifndef WOLFSSL_ESPIDF
    #warning "problem with wolfSSL user_settings. Check components/wolfssl/include"
#endif

#if ESP_IDF_VERSION_MAJOR >= 4
//    #include "protocol_examples_common.h"
#else
    const static int CONNECTED_BIT = BIT0;
    static EventGroupHandle_t wifi_event_group;
#endif

/* breadcrumb prefix for logging */
const static char *TAG = "tls_client";

#if ESP_IDF_VERSION_MAJOR < 4
/* event handler for wifi events */
static esp_err_t wifi_event_handler(void *ctx, system_event_t *event)
{
    switch (event->event_id)
    {
    case SYSTEM_EVENT_STA_START:
        esp_wifi_connect();
        break;
    case SYSTEM_EVENT_STA_GOT_IP:
    #if ESP_IDF_VERSION_MAJOR >= 4
        ESP_LOGI(TAG, "got ip:" IPSTR "\n",
                 IP2STR(&event->event_info.got_ip.ip_info.ip));
    #else
        ESP_LOGI(TAG, "got ip:%s",
                 ip4addr_ntoa(&event->event_info.got_ip.ip_info.ip));
    #endif
        /* see https://docs.espressif.com/projects/esp-idf/en/latest/esp32/api-reference/system/freertos_idf.html */
        xEventGroupSetBits(wifi_event_group, CONNECTED_BIT);
        break;
    case SYSTEM_EVENT_STA_DISCONNECTED:
        esp_wifi_connect();
        xEventGroupClearBits(wifi_event_group, CONNECTED_BIT);
        break;
    default:
        break;
    }
    return ESP_OK;
}
#else
#define EXAMPLE_ESP_WIFI_SSID      CONFIG_ESP_WIFI_SSID
#define EXAMPLE_ESP_WIFI_PASS      CONFIG_ESP_WIFI_PASSWORD

#ifdef CONFIG_ESP_MAXIMUM_RETRY
    #define EXAMPLE_ESP_MAXIMUM_RETRY  CONFIG_ESP_MAXIMUM_RETRY
#else
    #define CONFIG_ESP_MAXIMUM_RETRY 5
#endif


#if CONFIG_ESP_WIFI_AUTH_OPEN
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_OPEN
#elif CONFIG_ESP_WIFI_AUTH_WEP
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WEP
#elif CONFIG_ESP_WIFI_AUTH_WPA_PSK
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WPA_PSK
#elif CONFIG_ESP_WIFI_AUTH_WPA2_PSK
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WPA2_PSK
#elif CONFIG_ESP_WIFI_AUTH_WPA_WPA2_PSK
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WPA_WPA2_PSK
#elif CONFIG_ESP_WIFI_AUTH_WPA3_PSK
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WPA3_PSK
#elif CONFIG_ESP_WIFI_AUTH_WPA2_WPA3_PSK
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WPA2_WPA3_PSK
#elif CONFIG_ESP_WIFI_AUTH_WAPI_PSK
#define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD WIFI_AUTH_WAPI_PSK
#endif

#ifndef ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD
    #define CONFIG_ESP_WIFI_AUTH_WPA2_PSK 1
    #define ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD CONFIG_ESP_WIFI_AUTH_WPA2_PSK
#endif

/* FreeRTOS event group to signal when we are connected*/
static EventGroupHandle_t s_wifi_event_group;

/* The event group allows multiple bits for each event, but we only care about two events:
 * - we are connected to the AP with an IP
 * - we failed to connect after the maximum amount of retries */
#define WIFI_CONNECTED_BIT BIT0
#define WIFI_FAIL_BIT      BIT1


static int s_retry_num = 0;
ip_event_got_ip_t* event;


static void event_handler(void* arg, esp_event_base_t event_base,
                                int32_t event_id, void* event_data)
{
    if (event_base == WIFI_EVENT && event_id == WIFI_EVENT_STA_START) {
        esp_wifi_connect();
    } else if (event_base == WIFI_EVENT && event_id == WIFI_EVENT_STA_DISCONNECTED) {
        if (s_retry_num < EXAMPLE_ESP_MAXIMUM_RETRY) {
            esp_wifi_connect();
            s_retry_num++;
            ESP_LOGI(TAG, "retry to connect to the AP");
        } else {
            xEventGroupSetBits(s_wifi_event_group, WIFI_FAIL_BIT);
        }
        ESP_LOGI(TAG,"connect to the AP fail");
    } else if (event_base == IP_EVENT && event_id == IP_EVENT_STA_GOT_IP) {
        event = (ip_event_got_ip_t*) event_data;
        wifi_show_ip();
        s_retry_num = 0;
        xEventGroupSetBits(s_wifi_event_group, WIFI_CONNECTED_BIT);
    }
}

int wifi_init_sta(void)
{
    int ret = 0;
    s_wifi_event_group = xEventGroupCreate();

    ESP_ERROR_CHECK(esp_netif_init());

    ESP_ERROR_CHECK(esp_event_loop_create_default());
    esp_netif_create_default_wifi_sta();

    wifi_init_config_t cfg = WIFI_INIT_CONFIG_DEFAULT();
    ESP_ERROR_CHECK(esp_wifi_init(&cfg));

    esp_event_handler_instance_t instance_any_id;
    esp_event_handler_instance_t instance_got_ip;
    ESP_ERROR_CHECK(esp_event_handler_instance_register(WIFI_EVENT,
                                                        ESP_EVENT_ANY_ID,
                                                        &event_handler,
                                                        NULL,
                                                        &instance_any_id));
    ESP_ERROR_CHECK(esp_event_handler_instance_register(IP_EVENT,
                                                        IP_EVENT_STA_GOT_IP,
                                                        &event_handler,
                                                        NULL,
                                                        &instance_got_ip));

    wifi_config_t wifi_config = {
        .sta = {
            .ssid = EXAMPLE_ESP_WIFI_SSID,
            .password = EXAMPLE_ESP_WIFI_PASS,
            /* Authmode threshold resets to WPA2 as default if password matches
             * WPA2 standards (pasword len => 8). If you want to connect the
             * device to deprecated WEP/WPA networks, Please set the threshold
             * value WIFI_AUTH_WEP/WIFI_AUTH_WPA_PSK and set the password with
             * length and format matching to WIFI_AUTH_WEP/WIFI_AUTH_WPA_PSK
             * standards. */
            .threshold.authmode = ESP_WIFI_SCAN_AUTH_MODE_THRESHOLD,
            .sae_pwe_h2e = WPA3_SAE_PWE_BOTH,
        },
    };
    ESP_ERROR_CHECK(esp_wifi_set_mode(WIFI_MODE_STA) );
    ESP_ERROR_CHECK(esp_wifi_set_config(WIFI_IF_STA, &wifi_config) );
    ESP_ERROR_CHECK(esp_wifi_start() );

    ESP_LOGI(TAG, "wifi_init_sta finished.");

    /* Waiting until either the connection is established (WIFI_CONNECTED_BIT)
     * or connection failed for the maximum number of re-tries (WIFI_FAIL_BIT).
     * The bits are set by event_handler() (see above) */
    EventBits_t bits = xEventGroupWaitBits(s_wifi_event_group,
            WIFI_CONNECTED_BIT | WIFI_FAIL_BIT,
            pdFALSE,
            pdFALSE,
            portMAX_DELAY);

    /* xEventGroupWaitBits() returns the bits before the call returned,
     * hence we can test which event actually happened. */
#if defined(SHOW_SSID_AND_PASSWORD)
    ESP_LOGW(TAG, "Undefine SHOW_SSID_AND_PASSWORD to not show SSID/password");
    if (bits & WIFI_CONNECTED_BIT) {
        ESP_LOGI(TAG, "connected to ap SSID:%s password:%s",
                 EXAMPLE_ESP_WIFI_SSID, EXAMPLE_ESP_WIFI_PASS);
    } else if (bits & WIFI_FAIL_BIT) {
        ESP_LOGI(TAG, "Failed to connect to SSID:%s, password:%s",
                 EXAMPLE_ESP_WIFI_SSID, EXAMPLE_ESP_WIFI_PASS);
    } else {
        ESP_LOGE(TAG, "UNEXPECTED EVENT");
    }
#else
    if (bits & WIFI_CONNECTED_BIT) {
        ESP_LOGI(TAG, "Connected to AP");
    } else if (bits & WIFI_FAIL_BIT) {
        ESP_LOGI(TAG, "Failed to connect to AP");
        ret = -1;
    } else {
        ESP_LOGE(TAG, "Connect to AP UNEXPECTED EVENT");
        ret = -2;
    }
#endif
    return ret;
}

int wifi_show_ip(void)
{
    ESP_LOGI(TAG, "got ip:" IPSTR, IP2STR(&event->ip_info.ip));
    return 0;
}
#endif
