diff -cr --new-file src/smc_gen/r_bsp/mcu/all/resetprg.c src/smc_gen_A0/r_bsp/mcu/all/resetprg.c
*** src/smc_gen/r_bsp/mcu/all/resetprg.c	Tue Dec 13 14:52:54 2022
--- src/smc_gen_A0/r_bsp/mcu/all/resetprg.c	Tue Dec 13 14:57:16 2022
***************
*** 158,164 ****
  R_BSP_POR_FUNCTION(R_BSP_STARTUP_FUNCTION);
  
  /* Main program function declaration */
! #if (BSP_CFG_RTOS_USED == 0) || (BSP_CFG_RTOS_USED == 5)    /* Non-OS or Azure RTOS */
  extern void R_BSP_MAIN_FUNCTION(void);
  #endif
  
--- 158,164 ----
  R_BSP_POR_FUNCTION(R_BSP_STARTUP_FUNCTION);
  
  /* Main program function declaration */
! #if (BSP_CFG_RTOS_USED == 0) || (BSP_CFG_RTOS_USED == 5) || (BSP_CFG_RTOS_USED == 4)   /* Non-OS or Azure RTOS */
  extern void R_BSP_MAIN_FUNCTION(void);
  #endif
  
***************
*** 200,214 ****
       * and constructors of C++ objects have not been executed until the _INITSCT() is executed. */
  #if defined(__GNUC__)
  #if BSP_CFG_USER_STACK_ENABLE == 1
!     INTERNAL_NOT_USED(ustack_area);
  #endif
!     INTERNAL_NOT_USED(istack_area);
  #endif
  
  #if defined(__CCRX__) || defined(__GNUC__)
  
      /* Initialize the Interrupt Table Register */
!     R_BSP_SET_INTB(R_BSP_SECTOP_INTVECTTBL);
  
  #ifdef BSP_MCU_EXCEPTION_TABLE
      /* Initialize the Exception Table Register */
--- 200,214 ----
       * and constructors of C++ objects have not been executed until the _INITSCT() is executed. */
  #if defined(__GNUC__)
  #if BSP_CFG_USER_STACK_ENABLE == 1
!   //  INTERNAL_NOT_USED(ustack_area);
  #endif
!  //   INTERNAL_NOT_USED(istack_area);
  #endif
  
  #if defined(__CCRX__) || defined(__GNUC__)
  
      /* Initialize the Interrupt Table Register */
!  //   R_BSP_SET_INTB(R_BSP_SECTOP_INTVECTTBL);
  
  #ifdef BSP_MCU_EXCEPTION_TABLE
      /* Initialize the Exception Table Register */
***************
*** 275,281 ****
  #endif
  
      /* Initialize MCU interrupt callbacks. */
!     bsp_interrupt_open();
  
      /* Initialize register protection functionality. */
      bsp_register_protect_open();
--- 275,281 ----
  #endif
  
      /* Initialize MCU interrupt callbacks. */
!  //   bsp_interrupt_open();
  
      /* Initialize register protection functionality. */
      bsp_register_protect_open();
***************
*** 302,308 ****
      /* Enable the bus error interrupt to catch accesses to illegal/reserved areas of memory */
      R_BSP_InterruptControl(BSP_INT_SRC_BUS_ERROR, BSP_INT_CMD_INTERRUPT_ENABLE, FIT_NO_PTR);
  
! #if (BSP_CFG_RTOS_USED == 0) || (BSP_CFG_RTOS_USED == 5)    /* Non-OS or Azure RTOS */
      /* Call the main program function (should not return) */
      R_BSP_MAIN_FUNCTION();
  #elif BSP_CFG_RTOS_USED == 1    /* FreeRTOS */
--- 302,308 ----
      /* Enable the bus error interrupt to catch accesses to illegal/reserved areas of memory */
      R_BSP_InterruptControl(BSP_INT_SRC_BUS_ERROR, BSP_INT_CMD_INTERRUPT_ENABLE, FIT_NO_PTR);
  
! #if (BSP_CFG_RTOS_USED == 0) || (BSP_CFG_RTOS_USED == 5) || (BSP_CFG_RTOS_USED == 4)    /* Non-OS or Azure RTOS */
      /* Call the main program function (should not return) */
      R_BSP_MAIN_FUNCTION();
  #elif BSP_CFG_RTOS_USED == 1    /* FreeRTOS */
diff -cr --new-file src/smc_gen/r_config/r_bsp_config.h src/smc_gen_A0/r_config/r_bsp_config.h
*** src/smc_gen/r_config/r_bsp_config.h	Tue Dec 13 14:52:56 2022
--- src/smc_gen_A0/r_config/r_bsp_config.h	Tue Dec 13 14:57:16 2022
***************
*** 667,673 ****
     4 = Renesas ITRON OS (RI600V4 or RI600PX) is used.
     5 = Azure RTOS is used.(This is not available.)
  */
! #define BSP_CFG_RTOS_USED               (0)
  
  /* This macro is used to select which Renesas ITRON OS.
     0 = RI600V4 is used.
--- 667,673 ----
     4 = Renesas ITRON OS (RI600V4 or RI600PX) is used.
     5 = Azure RTOS is used.(This is not available.)
  */
! #define BSP_CFG_RTOS_USED               (4)
  
  /* This macro is used to select which Renesas ITRON OS.
     0 = RI600V4 is used.
diff -cr --new-file src/smc_gen/r_config/r_cmt_rx_config.h src/smc_gen_A0/r_config/r_cmt_rx_config.h
*** src/smc_gen/r_config/r_cmt_rx_config.h	Tue Dec 13 14:52:55 2022
--- src/smc_gen_A0/r_config/r_cmt_rx_config.h	Tue Dec 13 14:57:16 2022
***************
*** 37,43 ****
  #define CMT_RX_CFG_IPR         (5)
  
  #if (BSP_CFG_RTOS_USED == 4) && (BSP_CFG_RENESAS_RTOS_USED == 0) /* RI600V4 */
! #define _RI_TRACE_TIMER 1 /* RI600V4 uses CMT1 channel for the trace feature.*/
  #elif (BSP_CFG_RTOS_USED == 4) && (BSP_CFG_RENESAS_RTOS_USED == 1) /* RI600PX */
  #include "r_bsp_config.h"
  #define _RI_TRACE_TIMER BSP_CFG_RTOS_SYSTEM_TIMER /* RI600PX does not actually have the trace feature.*/
--- 37,43 ----
  #define CMT_RX_CFG_IPR         (5)
  
  #if (BSP_CFG_RTOS_USED == 4) && (BSP_CFG_RENESAS_RTOS_USED == 0) /* RI600V4 */
! #define _RI_TRACE_TIMER 0 /* RI600V4 uses CMT1 channel for the trace feature.*/
  #elif (BSP_CFG_RTOS_USED == 4) && (BSP_CFG_RENESAS_RTOS_USED == 1) /* RI600PX */
  #include "r_bsp_config.h"
  #define _RI_TRACE_TIMER BSP_CFG_RTOS_SYSTEM_TIMER /* RI600PX does not actually have the trace feature.*/
diff -cr --new-file src/smc_gen/r_t4_driver_rx/src/t4_driver.c src/smc_gen_A0/r_t4_driver_rx/src/t4_driver.c
*** src/smc_gen/r_t4_driver_rx/src/t4_driver.c	Tue Dec 13 15:19:38 2022
--- src/smc_gen_A0/r_t4_driver_rx/src/t4_driver.c	Tue Dec 13 14:57:17 2022
***************
*** 70,76 ****
  #include "r_tsip_rx_if.h"
  #elif (defined BSP_MCU_RX72M || defined BSP_MCU_RX72N || defined BSP_MCU_RX66N) && \
      (BSP_CFG_MCU_PART_FUNCTION == 0x11 /* H */)
! #include "r_tsip_rx_if.h"
  #else
  #warning "Your MCU does not support TSIP functions. It is better to use RX Family that support TSIP functions for more security. Vulnerability reference: https://www.ipa.go.jp/security/rfc/RFC1948EN.html"
  #endif  /* defined BSP_MCU_RX231 || defined BSP_MCU_RX23W && BSP_CFG_MCU_PART_VERSION == 0xB */
--- 70,76 ----
  #include "r_tsip_rx_if.h"
  #elif (defined BSP_MCU_RX72M || defined BSP_MCU_RX72N || defined BSP_MCU_RX66N) && \
      (BSP_CFG_MCU_PART_FUNCTION == 0x11 /* H */)
! //#include "r_tsip_rx_if.h"
  #else
  #warning "Your MCU does not support TSIP functions. It is better to use RX Family that support TSIP functions for more security. Vulnerability reference: https://www.ipa.go.jp/security/rfc/RFC1948EN.html"
  #endif  /* defined BSP_MCU_RX231 || defined BSP_MCU_RX23W && BSP_CFG_MCU_PART_VERSION == 0xB */
