From da37f7b051fe6833e25e78184cc9217dd4379187 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Mon, 23 Mar 2020 10:10:55 +0100
Subject: [PATCH] rpi-eeprom-update: OpenWrt defaults
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 rpi-eeprom-update         | 6 +++---
 rpi-eeprom-update-default | 5 +++--
 2 files changed, 6 insertions(+), 5 deletions(-)

--- a/rpi-eeprom-update
+++ b/rpi-eeprom-update
@@ -24,13 +24,13 @@ else
 fi
 
 # Selects the release sub-directory
-FIRMWARE_RELEASE_STATUS=${FIRMWARE_RELEASE_STATUS:-default}
+FIRMWARE_RELEASE_STATUS=${FIRMWARE_RELEASE_STATUS:-stable}
 FIRMWARE_IMAGE_DIR=${FIRMWARE_IMAGE_DIR:-${FIRMWARE_ROOT}/${FIRMWARE_RELEASE_STATUS}}
-FIRMWARE_BACKUP_DIR=${FIRMWARE_BACKUP_DIR:-/var/lib/raspberrypi/bootloader/backup}
+FIRMWARE_BACKUP_DIR=${FIRMWARE_BACKUP_DIR:-${FIRMWARE_ROOT}/backup}
 ENABLE_VL805_UPDATES=${ENABLE_VL805_UPDATES:-1}
 RECOVERY_BIN=${RECOVERY_BIN:-${FIRMWARE_ROOT}/${FIRMWARE_RELEASE_STATUS}/recovery.bin}
 BOOTFS=${BOOTFS:-/boot}
-VCMAILBOX=${VCMAILBOX:-/opt/vc/bin/vcmailbox}
+VCMAILBOX=${VCMAILBOX:-/usr/bin/vcmailbox}
 CM4_ENABLE_RPI_EEPROM_UPDATE=${CM4_ENABLE_RPI_EEPROM_UPDATE:-0}
 RPI_EEPROM_UPDATE_CONFIG_TOOL="${RPI_EEPROM_UPDATE_CONFIG_TOOL:-raspi-config}"
 
--- a/rpi-eeprom-update-default
+++ b/rpi-eeprom-update-default
@@ -1,8 +1,9 @@
 
 FIRMWARE_ROOT=/lib/firmware/raspberrypi/bootloader
-FIRMWARE_RELEASE_STATUS="critical"
+FIRMWARE_RELEASE_STATUS="stable"
 FIRMWARE_IMAGE_DIR="${FIRMWARE_ROOT}/${FIRMWARE_RELEASE_STATUS}"
-FIRMWARE_BACKUP_DIR="/var/lib/raspberrypi/bootloader/backup"
+FIRMWARE_BACKUP_DIR="${FIRMWARE_ROOT}/backup"
 BOOTFS=/boot
 USE_FLASHROM=0
 EEPROM_CONFIG_HOOK=
+VCMAILBOX=/usr/bin/vcmailbo
