diff --git a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
index 261827cdb957..13613f965a10 100644
--- a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -18,6 +18,10 @@
 		serial1 = &uart0;
 		mmc1 = &mmcnr;
 	};
+	memory@0 {
+		reg = <0x00 0x3c000000>;
+		device_type = "memory";
+	};
 };
 
 &gpio {
