# This file was generated using idf.py save-defconfig. It can be edited manually.
# Espressif IoT Development Framework (ESP-IDF) Project Minimal Configuration
#
CONFIG_PARTITION_TABLE_SINGLE_APP_LARGE=y
CONFIG_COMPILER_STACK_CHECK_MODE_ALL=y
CONFIG_ESP_TASK_WDT_CHECK_IDLE_TASK_CPU0=n
CONFIG_ESP_TASK_WDT_CHECK_IDLE_TASK_CPU1=n
CONFIG_LWIP_IPV6=n

CONFIG_FREERTOS_HZ=1000
CONFIG_ESP32_DEFAULT_CPU_FREQ_240=y

#
# Default main stack size
#
# This is typically way bigger than needed for stack size. See user_settings.h
#
CONFIG_ESP_MAIN_TASK_STACK_SIZE=55500
# Legacy stack size for older ESP-IDF versions
CONFIG_MAIN_TASK_STACK_SIZE=55500

#
# Compiler options
#
CONFIG_COMPILER_OPTIMIZATION_DEFAULT=y
CONFIG_COMPILER_OPTIMIZATION_ASSERTIONS_ENABLE=y
CONFIG_COMPILER_OPTIMIZATION_ASSERTION_LEVEL=2
CONFIG_COMPILER_HIDE_PATHS_MACROS=y
CONFIG_COMPILER_STACK_CHECK_MODE_NORM=y
CONFIG_COMPILER_STACK_CHECK=y

#
# Partition Table
#
# CONFIG_PARTITION_TABLE_SINGLE_APP is not set
CONFIG_PARTITION_TABLE_SINGLE_APP_LARGE=y
# CONFIG_PARTITION_TABLE_TWO_OTA is not set
# CONFIG_PARTITION_TABLE_CUSTOM is not set
CONFIG_PARTITION_TABLE_CUSTOM_FILENAME="partitions.csv"
CONFIG_PARTITION_TABLE_FILENAME="partitions_singleapp_large.csv"
CONFIG_PARTITION_TABLE_OFFSET=0x8000
CONFIG_PARTITION_TABLE_MD5=y
# end of Partition Table


CONFIG_FREERTOS_HZ=100
CONFIG_ESP_TASK_WDT_CHECK_IDLE_TASK_CPU0=1
CONFIG_ESP_TASK_WDT_CHECK_IDLE_TASK_CPU1=1
CONFIG_TASK_WDT_CHECK_IDLE_TASK_CPU0=CONFIG_ESP_TASK_WDT_CHECK_IDLE_TASK_CPU0
CONFIG_TASK_WDT_CHECK_IDLE_TASK_CPU1=CONFIG_ESP_TASK_WDT_CHECK_IDLE_TASK_CPU1
